
 ANSYS Multiphysics                                


 *------------------------------------------------------------------*
 |                                                                  |
 |   W E L C O M E   T O   T H E   A N S Y S (R)  P R O G R A M     |
 |                                                                  |
 *------------------------------------------------------------------*




 ***************************************************************
 *            ANSYS Release 18.0     LEGAL NOTICES             *
 ***************************************************************
 *                                                             *
 * Copyright 2016 SAS IP, Inc.  All rights reserved.           *
 * Unauthorized use, distribution or duplication is            *
 * prohibited.                                                 *
 *                                                             *
 * Ansys is a registered trademark of ANSYS, Inc. or its       *
 * subsidiaries in the United States or other countries.       *
 * See the ANSYS, Inc. online documentation or the ANSYS, Inc. *
 * documentation CD or online help for the complete Legal      *
 * Notice.                                                     *
 *                                                             *
 ***************************************************************
 *                                                             *
 * THIS ANSYS SOFTWARE PRODUCT AND PROGRAM DOCUMENTATION       *
 * INCLUDE TRADE SECRETS AND CONFIDENTIAL AND PROPRIETARY      *
 * PRODUCTS OF ANSYS, INC., ITS SUBSIDIARIES, OR LICENSORS.    *
 * The software products and documentation are furnished by    *
 * ANSYS, Inc. or its subsidiaries under a software license    *
 * agreement that contains provisions concerning               *
 * non-disclosure, copying, length and nature of use,          *
 * compliance with exporting laws, warranties, disclaimers,    *
 * limitations of liability, and remedies, and other           *
 * provisions.  The software products and documentation may be *
 * used, disclosed, transferred, or copied only in accordance  *
 * with the terms and conditions of that software license      *
 * agreement.                                                  *
 *                                                             *
 * ANSYS, Inc. is a UL registered                              *
 * ISO 9001:2008 company.                                      *
 *                                                             *
 ***************************************************************
 *                                                             *
 * This product is subject to U.S. laws governing export and   *
 * re-export.                                                  *
 *                                                             *
 * For U.S. Government users, except as specifically granted   *
 * by the ANSYS, Inc. software license agreement, the use,     *
 * duplication, or disclosure by the United States Government  *
 * is subject to restrictions stated in the ANSYS, Inc.        *
 * software license agreement and FAR 12.212 (for non-DOD      *
 * licenses).                                                  *
 *                                                             *
 ***************************************************************

 Release 18.0
     
 Point Releases and Patches installed:   
     
 ANSYS, Inc. Products Release 18.0   
 ANSYS Mechanical Products Release 18.0  
 ANSYS Autodyn Release 18.0  
 ANSYS LS-DYNA Release 18.0  
 ANSYS AIM Release 18.0  
 ANSYS CFX (includes ANSYS CFD-Post) Release 18.0
 ANSYS Fluent (includes ANSYS CFD-Post) Release 18.0 
 ANSYS TurboGrid Release 18.0
 ANSYS FENSAP-ICE Release 18.0   
 ANSYS Polyflow (includes ANSYS CFD-Post) Release 18.0   
 ANSYS Forte Release 18.0
 ANSYS Chemkin Release 18.0  
 ANSYS ICEM CFD Release 18.0 
 ANSYS Aqwa Release 18.0 
 ANSYS Icepak (includes ANSYS CFD-Post) Release 18.0 
 AutoCAD Release 18.0
 ACIS Release 18.0   
 Catia, Version 4 Release 18.0   
 Catia, Version 6 Release 18.0   
 Creo Elements/Direct Modeling Release 18.0  
 Inventor Release 18.0   
 JTOpen Release 18.0 
 NX Release 18.0 
 Parasolid Release 18.0  
 Creo Parametric (formerly Pro/ENGINEER) Release 18.0
 Solid Edge Release 18.0 
 SolidWorks Release 18.0 
 ANSYS, Inc. License Manager Release 18.0


          *****  ANSYS COMMAND LINE ARGUMENTS  *****
  BATCH MODE REQUESTED (-b)    = NOLIST
  INPUT FILE COPY MODE (-c)    = COPY
  DISTRIBUTED MEMORY PARALLEL REQUESTED
       2 PARALLEL PROCESSES REQUESTED WITH SINGLE THREAD PER PROCESS
    TOTAL OF     2 CORES REQUESTED
  MPI OPTION                   = INTELMPI
  INPUT FILE NAME              = G:\Study\Bolotov\popytka s boltami\_ProjectScratch\ScrE3BC\dummy.dat
  OUTPUT FILE NAME             = G:\Study\Bolotov\popytka s boltami\_ProjectScratch\ScrE3BC\solve.out
  START-UP FILE MODE           = NOREAD
  STOP FILE MODE               = NOREAD

 RELEASE= Release 18.0         BUILD= 18.0      UP20161219   VERSION=WINDOWS x64 
 CURRENT JOBNAME=file0  21:10:58  JUN 14, 2017 CP=      0.078


 PARAMETER _DS_PROGRESS =     999.0000000    

 /INPUT FILE= ds.dat  LINE=       0



 *** NOTE ***                            CP =       0.188   TIME= 21:10:58
 The /CONFIG,NOELDB command is not valid in a Distributed ANSYS          
 solution.  Command is ignored.                                          

 *GET  _WALLSTRT  FROM  ACTI  ITEM=TIME WALL  VALUE=  21.1827778    

 TITLE= 
 prostayay_poluchilas--Static Structural (A5)                                  


 SET PARAMETER DIMENSIONS ON  _WB_PROJECTSCRATCH_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_PROJECTSCRATCH_DIR(1) = G:\Study\Bolotov\popytka s boltami\_ProjectScratch\ScrE3BC\

 SET PARAMETER DIMENSIONS ON  _WB_SOLVERFILES_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_SOLVERFILES_DIR(1) = G:\Study\Bolotov\popytka s boltami\prostayay_poluchilas_files\dp0\global\MECH\SYS\Contact Tool\

 SET PARAMETER DIMENSIONS ON  _WB_USERFILES_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_USERFILES_DIR(1) = G:\Study\Bolotov\popytka s boltami\prostayay_poluchilas_files\user_files\
 --- Data in consistent MKS units. See Solving Units in the help system for more

 MKS UNITS SPECIFIED FOR INTERNAL    
  LENGTH        (l)  = METER (M)
  MASS          (M)  = KILOGRAM (KG)
  TIME          (t)  = SECOND (SEC)
  TEMPERATURE   (T)  = CELSIUS (C)
  TOFFSET            = 273.0
  CHARGE        (Q)  = COULOMB
  FORCE         (f)  = NEWTON (N) (KG-M/SEC2)
  HEAT               = JOULE (N-M)

  PRESSURE           = PASCAL (NEWTON/M**2)
  ENERGY        (W)  = JOULE (N-M)
  POWER         (P)  = WATT (N-M/SEC)
  CURRENT       (i)  = AMPERE (COULOMBS/SEC)
  CAPACITANCE   (C)  = FARAD
  INDUCTANCE    (L)  = HENRY
  MAGNETIC FLUX      = WEBER
  RESISTANCE    (R)  = OHM
  ELECTRIC POTENTIAL = VOLT

 INPUT  UNITS ARE ALSO SET TO MKS 

 *** ANSYS - ENGINEERING ANALYSIS SYSTEM  RELEASE Release 18.0     18.0     ***
 DISTRIBUTED ANSYS Multiphysics                                

 00000000  VERSION=WINDOWS x64   21:10:58  JUN 14, 2017 CP=      0.188

 prostayay_poluchilas--Static Structural (A5)                                  



          ***** ANSYS ANALYSIS DEFINITION (PREP7) *****
 *********** Nodes for the whole assembly ***********
 *********** Elements for Body 1 "Plita1" ***********
 *********** Elements for Body 2 "Plita2" ***********
 *********** Elements for Body 3 "Bolt" ***********
 *********** Elements for Body 4 "Gayka" ***********
 *********** Send User Defined Coordinate System(s) ***********
 *********** Send Materials ***********
 *********** Create Contact "Frictional - Gayka To Plita1" ***********
             Real Constant Set For Above Contact Is 6 & 5
 *********** Create Contact "Frictional - Bolt To Plita2" ***********
             Real Constant Set For Above Contact Is 8 & 7
 *********** Create Contact "Bonded - Gayka To Bolt" ***********
             Real Constant Set For Above Contact Is 10 & 9
 *********** Create Contact "Frictionless - Plita2 To Plita1" ***********
             Real Constant Set For Above Contact Is 12 & 11


 ***** ROUTINE COMPLETED *****  CP =         0.281


 --- Number of total nodes = 8677
 --- Number of contact elements = 2250
 --- Number of spring elements = 0
 --- Number of bearing elements = 0
 --- Number of solid elements = 2107
 --- Number of total elements = 4357

 *GET  _WALLBSOL  FROM  ACTI  ITEM=TIME WALL  VALUE=  21.1827778    

 *****  ANSYS SOLUTION ROUTINE  *****

 DO NOT SAVE ANY RESTART FILES AT ALL

 ERASE THE CURRENT DATABASE OUTPUT CONTROL TABLE.


 WRITE ALL  ITEMS TO THE DATABASE WITH A FREQUENCY OF NONE
   FOR ALL APPLICABLE ENTITIES

 WRITE NSOL ITEMS TO THE DATABASE WITH A FREQUENCY OF LAST
   FOR ALL APPLICABLE ENTITIES

 WRITE STRS ITEMS TO THE DATABASE WITH A FREQUENCY OF LAST
   FOR ALL APPLICABLE ENTITIES

 NLDIAG: Nonlinear diagnostics CONT option is set to ON. 
         Writing frequency : each ITERATION.

 CONTACT INFORMATION PRINTOUT LEVEL       1

 SELECT       FOR ITEM=ENAM COMPONENT=    
  IN RANGE       169 TO        175 STEP          1

       2250  ELEMENTS (OF       4357  DEFINED) SELECTED BY  ESEL  COMMAND.

 SELECT      ALL NODES HAVING ANY ELEMENT IN ELEMENT SET.

     3407 NODES (OF     8677  DEFINED) SELECTED FROM
     2250 SELECTED ELEMENTS BY NSLE COMMAND.

 SELECT      ALL ELEMENTS HAVING ANY NODE IN NODAL SET.

     3724 ELEMENTS (OF     4357  DEFINED) SELECTED FROM
     3407 SELECTED NODES BY  ESLN COMMAND.

 SELECT      ALL NODES HAVING ANY ELEMENT IN ELEMENT SET.

     7669 NODES (OF     8677  DEFINED) SELECTED FROM
     3724 SELECTED ELEMENTS BY NSLE COMMAND.

 CHECK INITIAL OPEN/CLOSED STATUS OF SELECTED CONTACT ELEMENTS
      AND POST INITIAL CONTACT STATUS

 *** SELECTION OF ELEMENT TECHNOLOGIES FOR APPLICABLE ELEMENTS ***
      --- GIVE SUGGESTIONS AND RESET THE KEY OPTIONS ---

 ELEMENT TYPE    1 IS SOLID186. KEYOPT(2) IS ALREADY SET AS SUGGESTED AND NO
 RESETTING IS NEEDED.

 ELEMENT TYPE    2 IS SOLID186. KEYOPT(2) IS ALREADY SET AS SUGGESTED AND NO
 RESETTING IS NEEDED.

 ELEMENT TYPE    3 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    4 IS SOLID186. KEYOPT(2) IS ALREADY SET AS SUGGESTED AND NO
 RESETTING IS NEEDED.



 *** NOTE ***                            CP =       0.281   TIME= 21:10:58
 This nonlinear analysis defaults to using the full Newton-Raphson       
 solution procedure.  This can be modified using the NROPT command.      

 SOLCONTROL,ON uses sparse matrix direct solver

 *** WARNING ***                         CP =       0.281   TIME= 21:10:58
 The program chosen initial timestep/load-factor is arbitrary.  It is    
 necessary for the user to supply a suitable initial                     
 timestep/load-factor through the NSUB or DELTIM command for             
 convergence and overall efficiency.                                     

 SOLUTION MONITORING INFO IS WRITTEN TO FILE= file.mntr                                                                                                                                                                                                                                                           

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 5 and contact element type 5 has been set up.  The         
 companion pair has real constant set ID 6.  Both pairs should have the  
 same behavior.                                                          
 For asymmetric contact analysis, you may keep the current pair and      
 deactivate its companion pair.                                          
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.24000E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16667E-03
 Max. initial friction coefficient MU         0.15000    
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.10000E-01
 The resulting elastic slip tolerance         0.16831E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.16831E-02
 Average contact pair depth                   0.16667E-02
 Default pinball region factor PINB            2.0000    
 The resulting pinball region                 0.33333E-02
 Initial penetration will be ramped during the first load step.

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Max.  Initial penetration 3.469446952E-18 was detected between contact  
 element 2171 and target element 2421.                                   
 ****************************************
  

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 6 and contact element type 5 has been set up.  The         
 companion pair has real constant set ID 5.  Both pairs should have the  
 same behavior.                                                          
 For asymmetric contact analysis, you may deactivate the current pair    
 and keep its companion pair.                                            
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.24000E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16667E-03
 Max. initial friction coefficient MU         0.15000    
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.10000E-01
 The resulting elastic slip tolerance         0.22457E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.22457E-02
 Average contact pair depth                   0.16667E-02
 Default pinball region factor PINB            2.0000    
 The resulting pinball region                 0.33333E-02
 Initial penetration will be ramped during the first load step.

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Max.  Initial penetration 3.469446952E-18 was detected between contact  
 element 2235 and target element 2126.                                   
 ****************************************
  

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 7 and contact element type 7 has been set up.  The         
 companion pair has real constant set ID 8.  Both pairs should have the  
 same behavior.                                                          
 For asymmetric contact analysis, you may keep the current pair and      
 deactivate its companion pair.                                          
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.20365E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.19642E-03
 Max. initial friction coefficient MU         0.15000    
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.10000E-01
 The resulting elastic slip tolerance         0.29643E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.29643E-02
 Average contact pair depth                   0.19642E-02
 Default pinball region factor PINB            2.0000    
 The resulting pinball region                 0.39283E-02
 Initial penetration will be ramped during the first load step.

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Max.  Initial penetration 0 was detected between contact element 2587   
 and target element 2821.                                                
 ****************************************
  

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 8 and contact element type 7 has been set up.  The         
 companion pair has real constant set ID 7.  Both pairs should have the  
 same behavior.                                                          
 For asymmetric contact analysis, you may deactivate the current pair    
 and keep its companion pair.                                            
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.20365E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16667E-03
 Max. initial friction coefficient MU         0.15000    
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.10000E-01
 The resulting elastic slip tolerance         0.22210E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.22210E-02
 Average contact pair depth                   0.16667E-02
 Default pinball region factor PINB            2.0000    
 The resulting pinball region                 0.33333E-02
 Initial penetration will be ramped during the first load step.

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Max.  Initial penetration 0 was detected between contact element 2636   
 and target element 2553.                                                
 ****************************************
  

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 9 and contact element type 9 has been set up.  The         
 companion pair has real constant set ID 10.  Both pairs should have     
 the same behavior.                                                      
 For asymmetric contact analysis, you may keep the current pair and      
 deactivate its companion pair.                                          
 Contact algorithm: Penalty method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.17765E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.13020E-03
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.84040E-05
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.16808E-02
 Average contact pair depth                   0.13020E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.32549E-03
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Max.  Initial penetration 9.244210119E-08 was detected between contact  
 element 3060 and target element 3559.                                   
 You may move entire target surface by : x= -6.138411946E-09, y=         
 9.32891801E-23, z= 9.223807225E-08,to reduce initial penetration.       
  
 Max.  Geometric gap 1.448134975E-06 has been detected between contact   
 element 3028 and target element 3624.                                   
 ****************************************
  

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 10 and contact element type 9 has been set up.  The        
 companion pair has real constant set ID 9.  Both pairs should have the  
 same behavior.                                                          
 For asymmetric contact analysis, you may deactivate the current pair    
 and keep its companion pair.                                            
 Contact algorithm: Penalty method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.17765E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.22517E-03
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.11879E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.23757E-02
 Average contact pair depth                   0.22517E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.56292E-03
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Max.  Initial penetration 6.855588682E-08 was detected between contact  
 element 3266 and target element 2995.                                   
 You may move entire target surface by : x= 4.26347619E-08, y=           
 1.254901699E-12, z= -5.368600091E-08,to reduce initial penetration.     
  
 Max.  Geometric gap 1.341981518E-06 has been detected between contact   
 element 3375 and target element 3014.                                   
 ****************************************
  

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 11 and contact element type 11 has been set up.  The       
 companion pair has real constant set ID 12.  Both pairs should have     
 the same behavior.                                                      
 For asymmetric contact analysis, you may keep the current pair and      
 deactivate its companion pair.                                          
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.24000E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16667E-03
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.22249E-02
 Average contact pair depth                   0.16667E-02
 Default pinball region factor PINB            2.0000    
 The resulting pinball region                 0.33333E-02
 Initial penetration will be ramped during the first load step.

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Min.  Initial gap 1.E-03 was detected between contact element 3925 and  
 target element 4274.                                                    
 You may move entire target surface by: x= 3.657016477E-19, y= 1.E-03,   
 z= -3.997946384E-19, to bring it in contact.                            
 ****************************************
  

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 12 and contact element type 11 has been set up.  The       
 companion pair has real constant set ID 11.  Both pairs should have     
 the same behavior.                                                      
 For asymmetric contact analysis, you may deactivate the current pair    
 and keep its companion pair.                                            
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.24000E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16667E-03
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.22552E-02
 Average contact pair depth                   0.16667E-02
 Default pinball region factor PINB            2.0000    
 The resulting pinball region                 0.33333E-02
 Initial penetration will be ramped during the first load step.

 *** NOTE ***                            CP =       0.562   TIME= 21:10:58
 Min.  Initial gap 1.E-03 was detected between contact element 4079 and  
 target element 3730.                                                    
 You may move entire target surface by: x= -1.098069445E-19, y= -1.E-03, 
 z= -2.055603803E-19, to bring it in contact.                            
 ****************************************
  
  
  

  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET           5
 Max.  Penetration of -3.469446952E-18 has been detected between contact 
 element 2182 and target element 2475.                                   
 For total 58 contact elements, there are 57 elements are in contact.    
 There are 57 elements are in sticking.                                  
 Contacting area 9.078539297E-05.                                        
 Max.  Pinball distance 3.33333334E-03.                                  
 One of the contact searching regions contains at least 23 target        
 elements.                                                               
 Max.  Pressure/force 8.085174362E-03.                                   
 Max.  Normal stiffness 2.330392848E+15.                                 
 Min.  Normal stiffness 2.330392848E+15.                                 
 Max.  Tangential stiffness 2.59609727E+14.                              
 Min.  Tangential stiffness 2.59609727E+14.                              
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET           6
 Max.  Penetration of -3.469446952E-18 has been detected between contact 
 element 2235 and target element 2126.                                   
 For total 160 contact elements, there are 33 elements are in contact.   
 There are 33 elements are in sticking.                                  
 Contacting area 1.208605463E-04.                                        
 Max.  Pinball distance 3.333333334E-03.                                 
 One of the contact searching regions contains at least 22 target        
 elements.                                                               
 Max.  Pressure/force 3.403974613E-03.                                   
 Max.  Normal stiffness 9.811288833E+14.                                 
 Min.  Normal stiffness 9.811288833E+14.                                 
 Max.  Tangential stiffness 8.1918789E+13.                               
 Min.  Tangential stiffness 8.1918789E+13.                               
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET           7
 Max.  Penetration of 0 has been detected between contact element 2611   
 and target element 2837.                                                
 For total 43 contact elements, there are 43 elements are in contact.    
 There are 43 elements are in sticking.                                  
 Contacting area 1.035461747E-04.                                        
 Max.  Pinball distance 3.928315888E-03.                                 
 One of the contact searching regions contains at least 36 target        
 elements.                                                               
 Max.  Pressure/force 1.559837663E-03.                                   
 Max.  Normal stiffness 5.924645572E+14.                                 
 Min.  Normal stiffness 5.924645572E+14.                                 
 Max.  Tangential stiffness 4.416461963E+13.                             
 Min.  Tangential stiffness 4.416461963E+13.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET           8
 Max.  Penetration of 0 has been detected between contact element 2672   
 and target element 2568.                                                
 For total 164 contact elements, there are 34 elements are in contact.   
 There are 34 elements are in sticking.                                  
 Contacting area 1.26002849E-04.                                         
 Max.  Pinball distance 3.333333334E-03.                                 
 One of the contact searching regions contains at least 19 target        
 elements.                                                               
 Max.  Pressure/force 1.697621545E-03.                                   
 Max.  Normal stiffness 8.605895656E+14.                                 
 Min.  Normal stiffness 8.605895656E+14.                                 
 Max.  Tangential stiffness 7.265286796E+13.                             
 Min.  Tangential stiffness 7.265286796E+13.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET           9
 Max.  Penetration of -9.03265592E-18 has been detected between contact  
 element 3040 and target element 3613.                                   
  
 Max.  Geometrical gap of 1.448134975E-06 has been detected between      
 contact element 3028 and target element 3624.                           
  
 Max.  Geometrical penetration of -9.244210119E-08 has been detected     
 between contact element 3028 and target element 3624.                   
 For total 60 contact elements, there are 60 elements are in contact.    
 There are 60 elements are in sticking.                                  
 Contacting area 1.727870128E-04.                                        
 Max.  Pinball distance 3.254881034E-04.                                 
 One of the contact searching regions contains at least 9 target         
 elements.                                                               
 Max.  Pressure/force 7.457603113E-03.                                   
 Max.  Normal stiffness 8.256268344E+14.                                 
 Min.  Normal stiffness 8.256268344E+14.                                 
 Max.  Tangential stiffness 4.796470714E+14.                             
 Min.  Tangential stiffness 4.796470714E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          10
 Max.  Penetration of -1.098894919E-17 has been detected between contact 
 element 3286 and target element 2992.                                   
  
 Max.  Geometrical gap of 1.341981518E-06 has been detected between      
 contact element 3375 and target element 3014.                           
  
 Max.  Geometrical penetration of -6.855588682E-08 has been detected     
 between contact element 3375 and target element 3014.                   
 For total 316 contact elements, there are 85 elements are in contact.   
 There are 85 elements are in sticking.                                  
 Contacting area 1.758897406E-04.                                        
 Max.  Pinball distance 5.629196405E-04.                                 
 One of the contact searching regions contains at least 9 target         
 elements.                                                               
 Max.  Pressure/force 1.661984614E-02.                                   
 Max.  Normal stiffness 1.512414504E+15.                                 
 Min.  Normal stiffness 1.512414504E+15.                                 
 Max.  Tangential stiffness 1.07507272E+15.                              
 Min.  Tangential stiffness 1.07507272E+15.                              
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          11
 Min.  Gap of 1.E-03 has been detected between contact element 3925 and  
 target element 4274.                                                    
 Max.  Pinball distance 3.333333334E-03.                                 
 One of the contact searching regions contains at least 32 target        
 elements.                                                               
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          12
 Min.  Gap of 1.E-03 has been detected between contact element 4079 and  
 target element 3730.                                                    
 Max.  Pinball distance 3.333333334E-03.                                 
 One of the contact searching regions contains at least 33 target        
 elements.                                                               
 *************************************************



            **** CENTER OF MASS, MASS, AND MASS MOMENTS OF INERTIA ****

  CALCULATIONS ASSUME ELEMENT MASS AT ELEMENT CENTROID

  TOTAL MASS =  0.58532E-01

                           MOM. OF INERTIA         MOM. OF INERTIA
  CENTER OF MASS            ABOUT ORIGIN        ABOUT CENTER OF MASS

  XC =  0.15018E-01      IXX =   0.2079E-04      IXX =   0.5162E-05
  YC = -0.64224E-02      IYY =   0.3383E-04      IYY =   0.7418E-05
  ZC =  0.15026E-01      IZZ =   0.2077E-04      IZZ =   0.5158E-05
                         IXY =   0.5638E-05      IXY =  -0.7771E-08
                         IYZ =   0.5641E-05      IYZ =  -0.7793E-08
                         IZX =  -0.1321E-04      IZX =  -0.8561E-09


  *** MASS SUMMARY BY ELEMENT TYPE ***

  TYPE      MASS
     1  0.205907E-01
     2  0.205907E-01
     3  0.144471E-01
     4  0.290361E-02

   *** ELEMENT MATRIX FORMULATION TIMES
     TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

        1       320  SOLID186      0.125   0.000391
        2       328  SOLID186      0.031   0.000095
        3       728  SOLID187      0.062   0.000086
        4        98  SOLID186      0.031   0.000319
        5       218  CONTA174      0.156   0.000717
        6       218  TARGE170      0.000   0.000000
        7       207  CONTA174      0.000   0.000000
        8       207  TARGE170      0.000   0.000000
        9       376  CONTA174      0.000   0.000000
       10       376  TARGE170      0.000   0.000000
       11       324  CONTA174      0.031   0.000096
       12       324  TARGE170      0.000   0.000000
 Time at end of element matrix formulation CP = 0.875.                   

   *** ELEMENT RESULT CALCULATION TIMES
     TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

        5       213  CONTA174      0.000   0.000000
        7       199  CONTA174      0.062   0.000314
        9       315  CONTA174      0.016   0.000050
       11       324  CONTA174      0.000   0.000000

   *** NODAL LOAD CALCULATION TIMES
     TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

        5       213  CONTA174      0.000   0.000000
        7       199  CONTA174      0.000   0.000000
        9       315  CONTA174      0.000   0.000000
       11       324  CONTA174      0.000   0.000000

 FINISH SOLUTION PROCESSING


 ***** ROUTINE COMPLETED *****  CP =         0.969



 *GET  _WALLASOL  FROM  ACTI  ITEM=TIME WALL  VALUE=  21.1827778    

 PRINTOUT RESUMED BY /GOP

 *GET  _WALLDONE  FROM  ACTI  ITEM=TIME WALL  VALUE=  21.1827778    

 PARAMETER _PREPTIME =     0.000000000    

 PARAMETER _SOLVTIME =     0.000000000    

 PARAMETER _POSTTIME =     0.000000000    

 PARAMETER _TOTALTIM =     0.000000000    

 EXIT ANSYS WITHOUT SAVING DATABASE


 NUMBER OF WARNING MESSAGES ENCOUNTERED=          1
 NUMBER OF ERROR   MESSAGES ENCOUNTERED=          0

+--------- D I S T R I B U T E D   A N S Y S   S T A T I S T I C S ------------+

Release: Release 18.0       Build: 18.0       Update: UP20161219   Platform: WINDOWS x64 
Date Run: 06/14/2017   Time: 21:10     Process ID: 5448
Operating System: Windows 10  (Build: 15063)

Processor Model: Intel(R) Core(TM) i5-4440 CPU @ 3.10GHz

Compiler: Intel(R) FORTRAN Compiler Version 15.0.7  (Build: 20160518)
          Intel(R) C/C++ Compiler Version 15.0.7  (Build: 20160518)
          Intel(R) Math Kernel Library Version 11.3.3 Product Build 20160413

Number of machines requested            :    1
Total number of cores available         :    4
Number of physical cores available      :    4
Number of processes requested           :    2
Number of threads per process requested :    1
Total number of cores requested         :    2 (Distributed Memory Parallel)               
MPI Type: INTELMPI
MPI Version: Intel(R) MPI Library 5.1.3 for Windows* OS


GPU Acceleration: Not Requested

Job Name: file0
Input File: dummy.dat

  Core                Machine Name   Working Directory
  ----------------------------------------------------
     0                   Goshik-PC   G:\Study\Bolotov\popytka s boltami\_ProjectScratch\ScrE3BC
     1                   Goshik-PC   G:\Study\Bolotov\popytka s boltami\_ProjectScratch\ScrE3BC
 
Latency time from master to core    1 =    0.710 microseconds
 
Communication speed from master to core    1 =  3447.33 MB/sec

Total CPU time for main thread                    :        0.6 seconds
Total CPU time summed for all threads             :        1.0 seconds

Elapsed time spent pre-processing model (/PREP7)  :        0.0 seconds
Elapsed time spent solution - preprocessing       :        0.0 seconds
Elapsed time spent computing solution             :        0.0 seconds
Elapsed time spent solution - postprocessing      :        0.0 seconds
Elapsed time spent post-processing model (/POST1) :        0.0 seconds
 
Equation solver used                              :            Sparse (symmetric)

Maximum total memory used                         :       27.0 MB
Maximum total memory allocated                    :     3136.0 MB
Total physical memory available                   :         16 GB

+------ E N D   D I S T R I B U T E D   A N S Y S   S T A T I S T I C S -------+


 *---------------------------------------------------------------------------*
 |                                                                           |
 |                       DISTRIBUTED ANSYS RUN COMPLETED                     |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 | Ansys Release 18.0          Build 18.0         UP20161219     WINDOWS x64 |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 | Database Requested(-db)  1024 MB    Scratch Memory Requested      1024 MB |
 | Maximum Database Used       7 MB    Maximum Scratch Memory Used     15 MB |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 |        CP Time      (sec) =          0.984       Time  =  21:10:58        |
 |        Elapsed Time (sec) =          2.000       Date  =  06/14/2017      |
 |                                                                           |
 *---------------------------------------------------------------------------*
