
 ANSYS Multiphysics                                


 *------------------------------------------------------------------*
 |                                                                  |
 |   W E L C O M E   T O   T H E   A N S Y S (R)  P R O G R A M     |
 |                                                                  |
 *------------------------------------------------------------------*




 ***************************************************************
 *            ANSYS Release 18.0     LEGAL NOTICES             *
 ***************************************************************
 *                                                             *
 * Copyright 2016 SAS IP, Inc.  All rights reserved.           *
 * Unauthorized use, distribution or duplication is            *
 * prohibited.                                                 *
 *                                                             *
 * Ansys is a registered trademark of ANSYS, Inc. or its       *
 * subsidiaries in the United States or other countries.       *
 * See the ANSYS, Inc. online documentation or the ANSYS, Inc. *
 * documentation CD or online help for the complete Legal      *
 * Notice.                                                     *
 *                                                             *
 ***************************************************************
 *                                                             *
 * THIS ANSYS SOFTWARE PRODUCT AND PROGRAM DOCUMENTATION       *
 * INCLUDE TRADE SECRETS AND CONFIDENTIAL AND PROPRIETARY      *
 * PRODUCTS OF ANSYS, INC., ITS SUBSIDIARIES, OR LICENSORS.    *
 * The software products and documentation are furnished by    *
 * ANSYS, Inc. or its subsidiaries under a software license    *
 * agreement that contains provisions concerning               *
 * non-disclosure, copying, length and nature of use,          *
 * compliance with exporting laws, warranties, disclaimers,    *
 * limitations of liability, and remedies, and other           *
 * provisions.  The software products and documentation may be *
 * used, disclosed, transferred, or copied only in accordance  *
 * with the terms and conditions of that software license      *
 * agreement.                                                  *
 *                                                             *
 * ANSYS, Inc. is a UL registered                              *
 * ISO 9001:2008 company.                                      *
 *                                                             *
 ***************************************************************
 *                                                             *
 * This product is subject to U.S. laws governing export and   *
 * re-export.                                                  *
 *                                                             *
 * For U.S. Government users, except as specifically granted   *
 * by the ANSYS, Inc. software license agreement, the use,     *
 * duplication, or disclosure by the United States Government  *
 * is subject to restrictions stated in the ANSYS, Inc.        *
 * software license agreement and FAR 12.212 (for non-DOD      *
 * licenses).                                                  *
 *                                                             *
 ***************************************************************

 Release 18.0
     
 Point Releases and Patches installed:   
     
 ANSYS, Inc. Products Release 18.0   
 ANSYS Mechanical Products Release 18.0  
 ANSYS Autodyn Release 18.0  
 ANSYS LS-DYNA Release 18.0  
 ANSYS AIM Release 18.0  
 ANSYS CFX (includes ANSYS CFD-Post) Release 18.0
 ANSYS Fluent (includes ANSYS CFD-Post) Release 18.0 
 ANSYS TurboGrid Release 18.0
 ANSYS FENSAP-ICE Release 18.0   
 ANSYS Polyflow (includes ANSYS CFD-Post) Release 18.0   
 ANSYS Forte Release 18.0
 ANSYS Chemkin Release 18.0  
 ANSYS ICEM CFD Release 18.0 
 ANSYS Aqwa Release 18.0 
 ANSYS Icepak (includes ANSYS CFD-Post) Release 18.0 
 AutoCAD Release 18.0
 ACIS Release 18.0   
 Catia, Version 4 Release 18.0   
 Catia, Version 6 Release 18.0   
 Creo Elements/Direct Modeling Release 18.0  
 Inventor Release 18.0   
 JTOpen Release 18.0 
 NX Release 18.0 
 Parasolid Release 18.0  
 Creo Parametric (formerly Pro/ENGINEER) Release 18.0
 Solid Edge Release 18.0 
 SolidWorks Release 18.0 
 ANSYS, Inc. License Manager Release 18.0


          *****  ANSYS COMMAND LINE ARGUMENTS  *****
  BATCH MODE REQUESTED (-b)    = NOLIST
  INPUT FILE COPY MODE (-c)    = COPY
  DISTRIBUTED MEMORY PARALLEL REQUESTED
       2 PARALLEL PROCESSES REQUESTED WITH SINGLE THREAD PER PROCESS
    TOTAL OF     2 CORES REQUESTED
  MPI OPTION                   = INTELMPI
  INPUT FILE NAME              = G:\Study\Bolotov\popytka s boltami\_ProjectScratch\ScrC022\dummy.dat
  OUTPUT FILE NAME             = G:\Study\Bolotov\popytka s boltami\_ProjectScratch\ScrC022\solve.out
  START-UP FILE MODE           = NOREAD
  STOP FILE MODE               = NOREAD

 RELEASE= Release 18.0         BUILD= 18.0      UP20161219   VERSION=WINDOWS x64 
 CURRENT JOBNAME=file0  20:21:40  JUN 14, 2017 CP=      0.078


 PARAMETER _DS_PROGRESS =     999.0000000    

 /INPUT FILE= ds.dat  LINE=       0



 *** NOTE ***                            CP =       0.203   TIME= 20:21:40
 The /CONFIG,NOELDB command is not valid in a Distributed ANSYS          
 solution.  Command is ignored.                                          

 *GET  _WALLSTRT  FROM  ACTI  ITEM=TIME WALL  VALUE=  20.3611111    

 TITLE= 
 prostayay_poluchilas--Static Structural (C5)                                  


 SET PARAMETER DIMENSIONS ON  _WB_PROJECTSCRATCH_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_PROJECTSCRATCH_DIR(1) = G:\Study\Bolotov\popytka s boltami\_ProjectScratch\ScrC022\

 SET PARAMETER DIMENSIONS ON  _WB_SOLVERFILES_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_SOLVERFILES_DIR(1) = G:\Study\Bolotov\popytka s boltami\prostayay_poluchilas_files\dp0\global\MECH\SYS-3\Contact Tool\

 SET PARAMETER DIMENSIONS ON  _WB_USERFILES_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_USERFILES_DIR(1) = G:\Study\Bolotov\popytka s boltami\prostayay_poluchilas_files\user_files\
 --- Data in consistent MKS units. See Solving Units in the help system for more

 MKS UNITS SPECIFIED FOR INTERNAL    
  LENGTH        (l)  = METER (M)
  MASS          (M)  = KILOGRAM (KG)
  TIME          (t)  = SECOND (SEC)
  TEMPERATURE   (T)  = CELSIUS (C)
  TOFFSET            = 273.0
  CHARGE        (Q)  = COULOMB
  FORCE         (f)  = NEWTON (N) (KG-M/SEC2)
  HEAT               = JOULE (N-M)

  PRESSURE           = PASCAL (NEWTON/M**2)
  ENERGY        (W)  = JOULE (N-M)
  POWER         (P)  = WATT (N-M/SEC)
  CURRENT       (i)  = AMPERE (COULOMBS/SEC)
  CAPACITANCE   (C)  = FARAD
  INDUCTANCE    (L)  = HENRY
  MAGNETIC FLUX      = WEBER
  RESISTANCE    (R)  = OHM
  ELECTRIC POTENTIAL = VOLT

 INPUT  UNITS ARE ALSO SET TO MKS 

 *** ANSYS - ENGINEERING ANALYSIS SYSTEM  RELEASE Release 18.0     18.0     ***
 DISTRIBUTED ANSYS Multiphysics                                

 00000000  VERSION=WINDOWS x64   20:21:40  JUN 14, 2017 CP=      0.203

 prostayay_poluchilas--Static Structural (C5)                                  



          ***** ANSYS ANALYSIS DEFINITION (PREP7) *****
 *********** Nodes for the whole assembly ***********
 *********** Elements for Body 1 "Plita1" ***********
 *********** Elements for Body 2 "Plita2" ***********
 *********** Elements for Body 3 "Bolt" ***********
 *********** Elements for Body 4 "Gayka" ***********
 *********** Send User Defined Coordinate System(s) ***********
 *********** Send Materials ***********
 *********** Create Contact "Frictional - Gayka To Plita1" ***********
             Real Constant Set For Above Contact Is 6 & 5
 *********** Create Contact "Frictional - Bolt To Plita2" ***********
             Real Constant Set For Above Contact Is 8 & 7
 *********** Create Contact "Bonded - Gayka To Bolt" ***********
             Real Constant Set For Above Contact Is 10 & 9
 *********** Create Contact "Frictional - Plita2 To Plita1" ***********
             Real Constant Set For Above Contact Is 12 & 11
 *********** Create Contact "Frictional - Plita1 To Plita2" ***********
             Real Constant Set For Above Contact Is 14 & 13


 ***** ROUTINE COMPLETED *****  CP =         0.266


 --- Number of total nodes = 7419
 --- Number of contact elements = 2444
 --- Number of spring elements = 0
 --- Number of bearing elements = 0
 --- Number of solid elements = 2557
 --- Number of total elements = 5001

 *GET  _WALLBSOL  FROM  ACTI  ITEM=TIME WALL  VALUE=  20.3611111    

 *****  ANSYS SOLUTION ROUTINE  *****

 DO NOT SAVE ANY RESTART FILES AT ALL

 ERASE THE CURRENT DATABASE OUTPUT CONTROL TABLE.


 WRITE ALL  ITEMS TO THE DATABASE WITH A FREQUENCY OF NONE
   FOR ALL APPLICABLE ENTITIES

 WRITE NSOL ITEMS TO THE DATABASE WITH A FREQUENCY OF LAST
   FOR ALL APPLICABLE ENTITIES

 WRITE STRS ITEMS TO THE DATABASE WITH A FREQUENCY OF LAST
   FOR ALL APPLICABLE ENTITIES

 NLDIAG: Nonlinear diagnostics CONT option is set to ON. 
         Writing frequency : each ITERATION.

 CONTACT INFORMATION PRINTOUT LEVEL       1

 SELECT       FOR ITEM=ENAM COMPONENT=    
  IN RANGE       169 TO        175 STEP          1

       2444  ELEMENTS (OF       5001  DEFINED) SELECTED BY  ESEL  COMMAND.

 SELECT      ALL NODES HAVING ANY ELEMENT IN ELEMENT SET.

     3242 NODES (OF     7419  DEFINED) SELECTED FROM
     2444 SELECTED ELEMENTS BY NSLE COMMAND.

 SELECT      ALL ELEMENTS HAVING ANY NODE IN NODAL SET.

     4601 ELEMENTS (OF     5001  DEFINED) SELECTED FROM
     3242 SELECTED NODES BY  ESLN COMMAND.

 SELECT      ALL NODES HAVING ANY ELEMENT IN ELEMENT SET.

     6794 NODES (OF     7419  DEFINED) SELECTED FROM
     4601 SELECTED ELEMENTS BY NSLE COMMAND.

 CHECK INITIAL OPEN/CLOSED STATUS OF SELECTED CONTACT ELEMENTS
      AND POST INITIAL CONTACT STATUS

 *** SELECTION OF ELEMENT TECHNOLOGIES FOR APPLICABLE ELEMENTS ***
      --- GIVE SUGGESTIONS AND RESET THE KEY OPTIONS ---

 ELEMENT TYPE    1 IS SOLID186. KEYOPT(2) IS ALREADY SET AS SUGGESTED AND NO
 RESETTING IS NEEDED.

 ELEMENT TYPE    2 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    3 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    4 IS SOLID186. KEYOPT(2) IS ALREADY SET AS SUGGESTED AND NO
 RESETTING IS NEEDED.



 *** NOTE ***                            CP =       0.328   TIME= 20:21:40
 This nonlinear analysis defaults to using the full Newton-Raphson       
 solution procedure.  This can be modified using the NROPT command.      

 SOLCONTROL,ON uses sparse matrix direct solver

 *** WARNING ***                         CP =       0.328   TIME= 20:21:40
 The program chosen initial timestep/load-factor is arbitrary.  It is    
 necessary for the user to supply a suitable initial                     
 timestep/load-factor through the NSUB or DELTIM command for             
 convergence and overall efficiency.                                     

 SOLUTION MONITORING INFO IS WRITTEN TO FILE= file.mntr                                                                                                                                                                                                                                                           

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 5 and contact element type 5 has been set up.  The         
 companion pair has real constant set ID 6.  Both pairs should have the  
 same behavior.                                                          
 For asymmetric contact analysis, you may keep the current pair and      
 deactivate its companion pair.                                          
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.24000E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16667E-03
 Max. initial friction coefficient MU         0.15000    
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.10000E-01
 The resulting elastic slip tolerance         0.18984E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.18984E-02
 Average contact pair depth                   0.16667E-02
 Default pinball region factor PINB            2.0000    
 The resulting pinball region                 0.33333E-02
 Initial penetration will be ramped during the first load step.

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Max.  Initial penetration 3.469446952E-18 was detected between contact  
 element 2609 and target element 2833.                                   
 ****************************************
  

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 6 and contact element type 5 has been set up.  The         
 companion pair has real constant set ID 5.  Both pairs should have the  
 same behavior.                                                          
 For asymmetric contact analysis, you may deactivate the current pair    
 and keep its companion pair.                                            
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.24000E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16667E-03
 Max. initial friction coefficient MU         0.15000    
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.10000E-01
 The resulting elastic slip tolerance         0.23545E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.23545E-02
 Average contact pair depth                   0.16667E-02
 Default pinball region factor PINB            2.0000    
 The resulting pinball region                 0.33333E-02
 Initial penetration will be ramped during the first load step.

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Max.  Initial penetration 3.469446952E-18 was detected between contact  
 element 2658 and target element 2598.                                   
 ****************************************
  

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 7 and contact element type 7 has been set up.  The         
 companion pair has real constant set ID 8.  Both pairs should have the  
 same behavior.                                                          
 For asymmetric contact analysis, you may keep the current pair and      
 deactivate its companion pair.                                          
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.12060E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.22105E-03
 Max. initial friction coefficient MU         0.15000    
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.10000E-01
 The resulting elastic slip tolerance         0.30155E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.30155E-02
 Average contact pair depth                   0.22105E-02
 Default pinball region factor PINB            2.0000    
 The resulting pinball region                 0.44209E-02
 Initial penetration will be ramped during the first load step.

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Max.  Initial penetration 0 was detected between contact element 2982   
 and target element 3249.                                                
 ****************************************
  

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 8 and contact element type 7 has been set up.  The         
 companion pair has real constant set ID 7.  Both pairs should have the  
 same behavior.                                                          
 For asymmetric contact analysis, you may deactivate the current pair    
 and keep its companion pair.                                            
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.12060E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.33166E-03
 Max. initial friction coefficient MU         0.15000    
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.10000E-01
 The resulting elastic slip tolerance         0.42717E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.42717E-02
 Average contact pair depth                   0.33166E-02
 Default pinball region factor PINB            2.0000    
 The resulting pinball region                 0.66333E-02
 Initial penetration will be ramped during the first load step.

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Max.  Initial penetration 0 was detected between contact element 3083   
 and target element 2980.                                                
 ****************************************
  

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 9 and contact element type 9 has been set up.  The         
 companion pair has real constant set ID 10.  Both pairs should have     
 the same behavior.                                                      
 For asymmetric contact analysis, you may keep the current pair and      
 deactivate its companion pair.                                          
 Contact algorithm: Penalty method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.16068E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.24894E-03
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.85252E-05
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.17050E-02
 Average contact pair depth                   0.24894E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.62236E-03
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Max.  Initial penetration 1.136015102E-07 was detected between contact  
 element 3438 and target element 3878.                                   
 You may move entire target surface by : x= -1.444669325E-09, y=         
 1.181600764E-22, z= 1.135923239E-07,to reduce initial penetration.      
  
 Max.  Geometric gap 1.140287561E-06 has been detected between contact   
 element 3431 and target element 3919.                                   
 ****************************************
  

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 10 and contact element type 9 has been set up.  The        
 companion pair has real constant set ID 9.  Both pairs should have the  
 same behavior.                                                          
 For asymmetric contact analysis, you may deactivate the current pair    
 and keep its companion pair.                                            
 Contact algorithm: Penalty method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.16068E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.24667E-03
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.12995E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.25990E-02
 Average contact pair depth                   0.24667E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.61669E-03
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Max.  Initial penetration 8.035020161E-08 was detected between contact  
 element 3626 and target element 3359.                                   
 You may move entire target surface by : x= 5.634716693E-08, y=          
 9.520100381E-13, z= 5.728133795E-08,to reduce initial penetration.      
  
 Max.  Geometric gap 1.133440569E-06 has been detected between contact   
 element 3653 and target element 3374.                                   
 ****************************************
  

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 11 and contact element type 11 has been set up.  The       
 companion pair has real constant set ID 12.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.12354E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.32378E-03
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.43115E-02
 Average contact pair depth                   0.32378E-02
 Default pinball region factor PINB            1.0000    
 The resulting pinball region                 0.32378E-02
 *WARNING*: Initial penetration is included.

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Min.  Initial gap 1.E-03 was detected between contact element 4093 and  
 target element 4469.                                                    
 You may move entire target surface by: x= 1.942890293E-19, y= 1.E-03,   
 z= -6.245004514E-20, to bring it in contact.                            
 ****************************************
  

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 12 and contact element type 11 has been set up.  The       
 companion pair has real constant set ID 11.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.12354E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16667E-03
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.23964E-02
 Average contact pair depth                   0.16667E-02
 Default pinball region factor PINB            1.0000    
 The resulting pinball region                 0.16667E-02
 *WARNING*: Initial penetration is included.

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Min.  Initial gap 1.E-03 was detected between contact element 4194 and  
 target element 4086.                                                    
 You may move entire target surface by: x= 6.269787867E-20, y= -1.E-03,  
 z= 2.483505315E-19, to bring it in contact.                             
 ****************************************
  

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 13 and contact element type 13 has been set up.  The       
 companion pair has real constant set ID 14.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.16862E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.23722E-03
 Max. initial friction coefficient MU         0.15000    
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.10000E-01
 The resulting elastic slip tolerance         0.20066E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.20066E-02
 Average contact pair depth                   0.23722E-02
 Default pinball region factor PINB            1.0000    
 The resulting pinball region                 0.23722E-02
 *WARNING*: Initial penetration is included.

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Max.  Initial penetration 6.938893904E-18 was detected between contact  
 element 4786 and target element 4996.                                   
 ****************************************
  

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 14 and contact element type 13 has been set up.  The       
 companion pair has real constant set ID 13.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  1.0000    
 The resulting initial contact stiffness      0.16862E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.21239E-03
 Max. initial friction coefficient MU         0.15000    
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.10000E-01
 The resulting elastic slip tolerance         0.44095E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.44095E-02
 Average contact pair depth                   0.21239E-02
 Default pinball region factor PINB            1.0000    
 The resulting pinball region                 0.21239E-02
 *WARNING*: Initial penetration is included.

 *** NOTE ***                            CP =       0.547   TIME= 20:21:40
 Max.  Initial penetration 6.938893904E-18 was detected between contact  
 element 4824 and target element 4554.                                   
 ****************************************
  
  
  

  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET           5
 Max.  Penetration of -3.469446952E-18 has been detected between contact 
 element 2647 and target element 2891.                                   
 For total 47 contact elements, there are 46 elements are in contact.    
 There are 46 elements are in sticking.                                  
 Contacting area 9.502473318E-05.                                        
 Max.  Pinball distance 3.33333334E-03.                                  
 One of the contact searching regions contains at least 24 target        
 elements.                                                               
 Max.  Pressure/force 5.634921272E-03.                                   
 Max.  Normal stiffness 1.624155478E+15.                                 
 Min.  Normal stiffness 1.624155478E+15.                                 
 Max.  Tangential stiffness 1.604176847E+14.                             
 Min.  Tangential stiffness 1.604176847E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET           6
 Max.  Penetration of -3.469446952E-18 has been detected between contact 
 element 2748 and target element 2604.                                   
 For total 145 contact elements, there are 30 elements are in contact.   
 There are 30 elements are in sticking.                                  
 Contacting area 1.254986856E-04.                                        
 Max.  Pinball distance 3.333333334E-03.                                 
 One of the contact searching regions contains at least 22 target        
 elements.                                                               
 Max.  Pressure/force 2.953395596E-03.                                   
 Max.  Normal stiffness 8.512583235E+14.                                 
 Min.  Normal stiffness 8.512583235E+14.                                 
 Max.  Tangential stiffness 6.778973519E+13.                             
 Min.  Tangential stiffness 6.778973519E+13.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET           7
 Max.  Penetration of 0 has been detected between contact element 3020   
 and target element 3241.                                                
 For total 40 contact elements, there are 40 elements are in contact.    
 There are 40 elements are in sticking.                                  
 Contacting area 1.176454917E-04.                                        
 Max.  Pinball distance 4.420910005E-03.                                 
 One of the contact searching regions contains at least 28 target        
 elements.                                                               
 Max.  Pressure/force 1.272316071E-03.                                   
 Max.  Normal stiffness 4.750500788E+14.                                 
 Min.  Normal stiffness 4.750500788E+14.                                 
 Max.  Tangential stiffness 3.917582887E+13.                             
 Min.  Tangential stiffness 3.917582887E+13.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET           8
 Max.  Penetration of 0 has been detected between contact element 3105   
 and target element 2981.                                                
 For total 158 contact elements, there are 28 elements are in contact.   
 There are 28 elements are in sticking.                                  
 Contacting area 1.021474868E-04.                                        
 Max.  Pinball distance 6.633296701E-03.                                 
 One of the contact searching regions contains at least 34 target        
 elements.                                                               
 Max.  Pressure/force 2.141715254E-03.                                   
 Max.  Normal stiffness 5.644985702E+14.                                 
 Min.  Normal stiffness 5.644985702E+14.                                 
 Max.  Tangential stiffness 4.93078572E+13.                              
 Min.  Tangential stiffness 4.93078572E+13.                              
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET           9
 Max.  Penetration of -1.431582469E-17 has been detected between contact 
 element 3428 and target element 3856.                                   
  
 Max.  Geometrical gap of 1.140287561E-06 has been detected between      
 contact element 3431 and target element 3919.                           
  
 Max.  Geometrical penetration of -1.136015102E-07 has been detected     
 between contact element 3431 and target element 3919.                   
 For total 57 contact elements, there are 57 elements are in contact.    
 There are 57 elements are in sticking.                                  
 Contacting area 1.727868802E-04.                                        
 Max.  Pinball distance 6.223606512E-04.                                 
 One of the contact searching regions contains at least 13 target        
 elements.                                                               
 Max.  Pressure/force 2.300245792E-02.                                   
 Max.  Normal stiffness 1.606785387E+15.                                 
 Min.  Normal stiffness 1.606785387E+15.                                 
 Max.  Tangential stiffness 1.759493906E+15.                             
 Min.  Tangential stiffness 1.759493906E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          10
 Max.  Penetration of -7.846353124E-18 has been detected between contact 
 element 3650 and target element 3364.                                   
  
 Max.  Geometrical gap of 1.133440569E-06 has been detected between      
 contact element 3653 and target element 3374.                           
  
 Max.  Geometrical penetration of -8.035020161E-08 has been detected     
 between contact element 3653 and target element 3374.                   
 For total 266 contact elements, there are 81 elements are in contact.   
 There are 81 elements are in sticking.                                  
 Contacting area 1.733871958E-04.                                        
 Max.  Pinball distance 6.166860322E-04.                                 
 One of the contact searching regions contains at least 9 target         
 elements.                                                               
 Max.  Pressure/force -1.106687798E-02.                                  
 Max.  Normal stiffness 1.373778959E+15.                                 
 Min.  Normal stiffness 1.373778959E+15.                                 
 Max.  Tangential stiffness 9.779075209E+14.                             
 Min.  Tangential stiffness 9.779075209E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          11

 *** NOTE ***                            CP =       0.844   TIME= 20:21:40
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          12
 Min.  Gap of 1.E-03 has been detected between contact element 4300 and  
 target element 3993.                                                    
 Max.  Pinball distance 1.666666667E-03.                                 
 One of the contact searching regions contains at least 17 target        
 elements.                                                               
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          13
 Max.  Penetration of -6.938893904E-18 has been detected between contact 
 element 4786 and target element 4996.                                   
 For total 156 contact elements, there are 156 elements are in contact.  
 There are 156 elements are in sticking.                                 
 Contacting area 4.903846158E-04.                                        
 Max.  Pinball distance 2.37217488E-03.                                  
 One of the contact searching regions contains at least 14 target        
 elements.                                                               
 Max.  Pressure/force 1.170047616E-02.                                   
 Max.  Normal stiffness 1.686216322E+15.                                 
 Min.  Normal stiffness 1.686216322E+15.                                 
 Max.  Tangential stiffness 2.242605077E+14.                             
 Min.  Tangential stiffness 2.242605077E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          14

 *** NOTE ***                            CP =       0.844   TIME= 20:21:40
 Contact pair is inactive.                                               



            **** CENTER OF MASS, MASS, AND MASS MOMENTS OF INERTIA ****

  CALCULATIONS ASSUME ELEMENT MASS AT ELEMENT CENTROID

  TOTAL MASS =  0.10327    

                           MOM. OF INERTIA         MOM. OF INERTIA
  CENTER OF MASS            ABOUT ORIGIN        ABOUT CENTER OF MASS

  XC =  0.14955E-01      IXX =   0.3896E-04      IXX =   0.1230E-04
  YC = -0.57953E-02      IYY =   0.6687E-04      IYY =   0.2059E-04
  ZC =  0.14986E-01      IZZ =   0.3882E-04      IZZ =   0.1226E-04
                         IXY =   0.8932E-05      IXY =  -0.1778E-07
                         IYZ =   0.8974E-05      IYZ =   0.5985E-08
                         IZX =  -0.2316E-04      IZX =  -0.1451E-07


  *** MASS SUMMARY BY ELEMENT TYPE ***

  TYPE      MASS
     1  0.240369E-01
     2  0.599184E-01
     3  0.152756E-01
     4  0.403418E-02

   *** ELEMENT MATRIX FORMULATION TIMES
     TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

        1       338  SOLID186      0.031   0.000092
        2      1118  SOLID187      0.125   0.000112
        3       614  SOLID187      0.078   0.000127
        4        87  SOLID186      0.000   0.000000
        5       192  CONTA174      0.000   0.000000
        6       192  TARGE170      0.000   0.000000
        7       198  CONTA174      0.125   0.000631
        8       198  TARGE170      0.000   0.000000
        9       323  CONTA174      0.047   0.000145
       10       323  TARGE170      0.000   0.000000
       11       249  CONTA174      0.000   0.000000
       12       249  TARGE170      0.000   0.000000
       13       260  CONTA174      0.000   0.000000
       14       260  TARGE170      0.000   0.000000
 Time at end of element matrix formulation CP = 0.84375.                 

   *** ELEMENT RESULT CALCULATION TIMES
     TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

        5       192  CONTA174      0.062   0.000326
        7       198  CONTA174      0.031   0.000158
        9       281  CONTA174      0.000   0.000000
       11       249  CONTA174      0.031   0.000126
       13       260  CONTA174      0.000   0.000000

   *** NODAL LOAD CALCULATION TIMES
     TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

        5       192  CONTA174      0.000   0.000000
        7       198  CONTA174      0.000   0.000000
        9       281  CONTA174      0.000   0.000000
       11       249  CONTA174      0.000   0.000000
       13       260  CONTA174      0.000   0.000000

 FINISH SOLUTION PROCESSING


 ***** ROUTINE COMPLETED *****  CP =         0.953



 *GET  _WALLASOL  FROM  ACTI  ITEM=TIME WALL  VALUE=  20.3611111    

 PRINTOUT RESUMED BY /GOP

 *GET  _WALLDONE  FROM  ACTI  ITEM=TIME WALL  VALUE=  20.3611111    

 PARAMETER _PREPTIME =     0.000000000    

 PARAMETER _SOLVTIME =     0.000000000    

 PARAMETER _POSTTIME =     0.000000000    

 PARAMETER _TOTALTIM =     0.000000000    

 EXIT ANSYS WITHOUT SAVING DATABASE


 NUMBER OF WARNING MESSAGES ENCOUNTERED=          1
 NUMBER OF ERROR   MESSAGES ENCOUNTERED=          0

+--------- D I S T R I B U T E D   A N S Y S   S T A T I S T I C S ------------+

Release: Release 18.0       Build: 18.0       Update: UP20161219   Platform: WINDOWS x64 
Date Run: 06/14/2017   Time: 20:21     Process ID: 12668
Operating System: Windows 10  (Build: 15063)

Processor Model: Intel(R) Core(TM) i5-4440 CPU @ 3.10GHz

Compiler: Intel(R) FORTRAN Compiler Version 15.0.7  (Build: 20160518)
          Intel(R) C/C++ Compiler Version 15.0.7  (Build: 20160518)
          Intel(R) Math Kernel Library Version 11.3.3 Product Build 20160413

Number of machines requested            :    1
Total number of cores available         :    4
Number of physical cores available      :    4
Number of processes requested           :    2
Number of threads per process requested :    1
Total number of cores requested         :    2 (Distributed Memory Parallel)               
MPI Type: INTELMPI
MPI Version: Intel(R) MPI Library 5.1.3 for Windows* OS


GPU Acceleration: Not Requested

Job Name: file0
Input File: dummy.dat

  Core                Machine Name   Working Directory
  ----------------------------------------------------
     0                   Goshik-PC   G:\Study\Bolotov\popytka s boltami\_ProjectScratch\ScrC022
     1                   Goshik-PC   G:\Study\Bolotov\popytka s boltami\_ProjectScratch\ScrC022
 
Latency time from master to core    1 =    0.650 microseconds
 
Communication speed from master to core    1 =  3725.73 MB/sec

Total CPU time for main thread                    :        0.6 seconds
Total CPU time summed for all threads             :        1.0 seconds

Elapsed time spent pre-processing model (/PREP7)  :        0.0 seconds
Elapsed time spent solution - preprocessing       :        0.0 seconds
Elapsed time spent computing solution             :        0.0 seconds
Elapsed time spent solution - postprocessing      :        0.0 seconds
Elapsed time spent post-processing model (/POST1) :        0.0 seconds
 
Equation solver used                              :            Sparse (symmetric)

Maximum total memory used                         :       27.0 MB
Maximum total memory allocated                    :     3136.0 MB
Total physical memory available                   :         16 GB

+------ E N D   D I S T R I B U T E D   A N S Y S   S T A T I S T I C S -------+


 *---------------------------------------------------------------------------*
 |                                                                           |
 |                       DISTRIBUTED ANSYS RUN COMPLETED                     |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 | Ansys Release 18.0          Build 18.0         UP20161219     WINDOWS x64 |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 | Database Requested(-db)  1024 MB    Scratch Memory Requested      1024 MB |
 | Maximum Database Used       7 MB    Maximum Scratch Memory Used     15 MB |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 |        CP Time      (sec) =          0.969       Time  =  20:21:40        |
 |        Elapsed Time (sec) =          2.000       Date  =  06/14/2017      |
 |                                                                           |
 *---------------------------------------------------------------------------*
