
 ANSYS Multiphysics                                


 *------------------------------------------------------------------*
 |                                                                  |
 |   W E L C O M E   T O   T H E   A N S Y S (R)  P R O G R A M     |
 |                                                                  |
 *------------------------------------------------------------------*




 ***************************************************************
 *            ANSYS Release 18.1     LEGAL NOTICES             *
 ***************************************************************
 *                                                             *
 * Copyright 2017 SAS IP, Inc.  All rights reserved.           *
 * Unauthorized use, distribution or duplication is            *
 * prohibited.                                                 *
 *                                                             *
 * Ansys is a registered trademark of ANSYS, Inc. or its       *
 * subsidiaries in the United States or other countries.       *
 * See the ANSYS, Inc. online documentation or the ANSYS, Inc. *
 * documentation CD or online help for the complete Legal      *
 * Notice.                                                     *
 *                                                             *
 ***************************************************************
 *                                                             *
 * THIS ANSYS SOFTWARE PRODUCT AND PROGRAM DOCUMENTATION       *
 * INCLUDE TRADE SECRETS AND CONFIDENTIAL AND PROPRIETARY      *
 * PRODUCTS OF ANSYS, INC., ITS SUBSIDIARIES, OR LICENSORS.    *
 * The software products and documentation are furnished by    *
 * ANSYS, Inc. or its subsidiaries under a software license    *
 * agreement that contains provisions concerning               *
 * non-disclosure, copying, length and nature of use,          *
 * compliance with exporting laws, warranties, disclaimers,    *
 * limitations of liability, and remedies, and other           *
 * provisions.  The software products and documentation may be *
 * used, disclosed, transferred, or copied only in accordance  *
 * with the terms and conditions of that software license      *
 * agreement.                                                  *
 *                                                             *
 * ANSYS, Inc. is a UL registered                              *
 * ISO 9001:2008 company.                                      *
 *                                                             *
 ***************************************************************
 *                                                             *
 * This product is subject to U.S. laws governing export and   *
 * re-export.                                                  *
 *                                                             *
 * For U.S. Government users, except as specifically granted   *
 * by the ANSYS, Inc. software license agreement, the use,     *
 * duplication, or disclosure by the United States Government  *
 * is subject to restrictions stated in the ANSYS, Inc.        *
 * software license agreement and FAR 12.212 (for non-DOD      *
 * licenses).                                                  *
 *                                                             *
 ***************************************************************

 Release 18.1
     
 Point Releases and Patches installed:   
     
 ANSYS, Inc. Products Release 18.1   
 ANSYS Mechanical Products Release 18.1  
 ANSYS Autodyn Release 18.1  
 ANSYS LS-DYNA Release 18.1  
 ANSYS AIM Release 18.1  
 ANSYS CFX (includes ANSYS CFD-Post) Release 18.1
 ANSYS Fluent (includes ANSYS CFD-Post) Release 18.1 
 ANSYS TurboGrid Release 18.1
 ANSYS FENSAP-ICE Release 18.1   
 ANSYS Polyflow (includes ANSYS CFD-Post) Release 18.1   
 ANSYS Forte Release 18.1
 ANSYS Chemkin Release 18.1  
 ANSYS ICEM CFD Release 18.1 
 ANSYS Aqwa Release 18.1 
 ANSYS Icepak (includes ANSYS CFD-Post) Release 18.1 
 AutoCAD Release 18.1
 ACIS Release 18.1   
 Catia, Version 4 Release 18.1   
 Catia, Version 6 Release 18.1   
 Creo Elements/Direct Modeling Release 18.1  
 Inventor Release 18.1   
 JTOpen Release 18.1 
 NX Release 18.1 
 Parasolid Release 18.1  
 Creo Parametric Release 18.1
 Solid Edge Release 18.1 
 SolidWorks Release 18.1 
 ANSYS, Inc. License Manager Release 18.1


          *****  ANSYS COMMAND LINE ARGUMENTS  *****
  BATCH MODE REQUESTED (-b)    = NOLIST
  INPUT FILE COPY MODE (-c)    = COPY
  DISTRIBUTED MEMORY PARALLEL REQUESTED
       2 PARALLEL PROCESSES REQUESTED WITH SINGLE THREAD PER PROCESS
    TOTAL OF     2 CORES REQUESTED
  MPI OPTION                   = INTELMPI
  INPUT FILE NAME              = C:\Users\azer.b\AppData\Local\Temp\WB_OLEG-WS_Oleg.g_5632_2\_ProjectScratch\ScrC268\dummy.dat
  OUTPUT FILE NAME             = C:\Users\azer.b\AppData\Local\Temp\WB_OLEG-WS_Oleg.g_5632_2\_ProjectScratch\ScrC268\solve.out
  START-UP FILE MODE           = NOREAD
  STOP FILE MODE               = NOREAD

 RELEASE= Release 18.1         BUILD= 18.1      UP20170403   VERSION=WINDOWS x64 
 CURRENT JOBNAME=file0  18:56:33  SEP 12, 2017 CP=      0.141


 PARAMETER _DS_PROGRESS =     999.0000000    

 /INPUT FILE= ds.dat  LINE=       0



 *** NOTE ***                            CP =       0.250   TIME= 18:56:33
 The /CONFIG,NOELDB command is not valid in a Distributed ANSYS          
 solution.  Command is ignored.                                          

 *GET  _WALLSTRT  FROM  ACTI  ITEM=TIME WALL  VALUE=  18.9425000    

 TITLE= 
 unsaved_project--Static Structural (C5)                                       

  ACT Extensions:
      MechanicalDropTest, 2.0
      f0fd899f-9d88-4f46-8cf1-36bf5c218d65, wbex
  

 SET PARAMETER DIMENSIONS ON  _WB_PROJECTSCRATCH_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_PROJECTSCRATCH_DIR(1) = C:\Users\azer.b\AppData\Local\Temp\WB_OLEG-WS_Oleg.g_5632_2\_ProjectScratch\ScrC268\

 SET PARAMETER DIMENSIONS ON  _WB_SOLVERFILES_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_SOLVERFILES_DIR(1) = C:\Users\azer.b\AppData\Local\Temp\WB_OLEG-WS_Oleg.g_5632_2\unsaved_project_files\dp0\SYS-3\MECH\

 SET PARAMETER DIMENSIONS ON  _WB_USERFILES_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_USERFILES_DIR(1) = C:\Users\azer.b\AppData\Local\Temp\WB_OLEG-WS_Oleg.g_5632_2\unsaved_project_files\user_files\
 --- Data in consistent NMM units. See Solving Units in the help system for more

 MPA UNITS SPECIFIED FOR INTERNAL    
  LENGTH      = MILLIMETERS (mm)
  MASS        = TONNE (Mg)
  TIME        = SECONDS (sec)
  TEMPERATURE = CELSIUS (C)
  TOFFSET     = 273.0
  FORCE       = NEWTON (N)
  HEAT        = MILLIJOULES (mJ)

 INPUT  UNITS ARE ALSO SET TO MPA 

 *** ANSYS - ENGINEERING ANALYSIS SYSTEM  RELEASE Release 18.1     18.1     ***
 DISTRIBUTED ANSYS Multiphysics                                

 00000000  VERSION=WINDOWS x64   18:56:33  SEP 12, 2017 CP=      0.250

 unsaved_project--Static Structural (C5)                                       



          ***** ANSYS ANALYSIS DEFINITION (PREP7) *****
 *********** Nodes for the whole assembly ***********
 *********** Elements for Body 1 "Part 1" ***********
 *********** Elements for Body 2 "Part 2" ***********
 *********** Elements for Body 3 "Part 3" ***********
 *********** Elements for Body 4 "Part 4" ***********
 *********** Elements for Body 5 "Part 5" ***********
 *********** Elements for Body 6 "Part 6" ***********
 *********** Elements for Body 7 "Part 7" ***********
 *********** Elements for Body 8 "Part 8" ***********
 *********** Elements for Body 9 "bolt_type_anchor_shackles_1019677_Temp_1" ****
 *********** Elements for Body 10 "bolt_type_anchor_shackles_1019677_Temp_2" ***
 *********** Send User Defined Coordinate System(s) ***********
 *********** Set Reference Temperature ***********
 *********** Send Materials ***********
 *********** Create Contact "Contact Region" ***********
             Real Constant Set For Above Contact Is 12 & 11
 *********** Create Contact "Contact Region 2" ***********
             Real Constant Set For Above Contact Is 14 & 13
 *********** Create Contact "Contact Region 3" ***********
             Real Constant Set For Above Contact Is 16 & 15
 *********** Create Contact "Contact Region 4" ***********
             Real Constant Set For Above Contact Is 18 & 17
 *********** Create Contact "Contact Region 5" ***********
             Real Constant Set For Above Contact Is 20 & 19
 *********** Create Contact "Contact Region 6" ***********
             Real Constant Set For Above Contact Is 22 & 21
 *********** Create Contact "Contact Region 7" ***********
             Real Constant Set For Above Contact Is 24 & 23
 *********** Create Contact "Contact Region 8" ***********
             Real Constant Set For Above Contact Is 26 & 25
 *********** Create Contact "Contact Region 9" ***********
             Real Constant Set For Above Contact Is 28 & 27
 *********** Create Contact "Contact Region 10" ***********
             Real Constant Set For Above Contact Is 30 & 29
 *********** Create Contact "Contact Region 11" ***********
             Real Constant Set For Above Contact Is 32 & 31
 *********** Create Contact "Contact Region 16" ***********
             Real Constant Set For Above Contact Is 34 & 33
 *********** Create Contact "Contact Region 18" ***********
             Real Constant Set For Above Contact Is 36 & 35
 *********** Create Contact "Contact Region 19" ***********
             Real Constant Set For Above Contact Is 38 & 37
 *********** Create Contact "Contact Region 20" ***********
             Real Constant Set For Above Contact Is 40 & 39
 *********** Create Contact "Contact Region 21" ***********
             Real Constant Set For Above Contact Is 42 & 41
 *********** Create Contact "Contact Region 22" ***********
             Real Constant Set For Above Contact Is 44 & 43
 *********** Fixed Supports ***********
 *********** Define Force Using Surface Effect Elements ***********


 ***** ROUTINE COMPLETED *****  CP =         0.781


 --- Number of total nodes = 77114
 --- Number of contact elements = 8656
 --- Number of spring elements = 0
 --- Number of bearing elements = 0
 --- Number of solid elements = 20651
 --- Number of condensed parts = 0
 --- Number of total elements = 29307

 *GET  _WALLBSOL  FROM  ACTI  ITEM=TIME WALL  VALUE=  18.9425000    
 ****************************************************************************
 *************************    SOLUTION       ********************************
 ****************************************************************************

 *****  ANSYS SOLUTION ROUTINE  *****


 PERFORM A STATIC ANALYSIS
  THIS WILL BE A NEW ANALYSIS

 USE A MAXIMUM OF     1 EQUILIBRIUM ITERATIONS EACH SUBSTEP

 *** WARNING ***                         CP =       0.781   TIME= 18:56:33
 Using 1 iteration per substep may result in unconverged solutions for   
 nonlinear analysis and the program may not indicate divergence in this  
 case.  Check your results.                                              

 DO NOT USE PREDICTOR METHOD FOR  ALL DEGREES OF FREEDOM

 USE SPARSE MATRIX DIRECT SOLVER

 CONTACT INFORMATION PRINTOUT LEVEL       1

 DO NOT COMBINE ELEMENT MATRIX FILES (.emat) AFTER DISTRIBUTED PARALLEL SOLUTION

 DO NOT COMBINE ELEMENT SAVE DATA FILES (.esav) AFTER DISTRIBUTED PARALLEL SOLUTION

 NLDIAG: Nonlinear diagnostics CONT option is set to ON. 
         Writing frequency : each ITERATION.

 DO NOT SAVE ANY RESTART FILES AT ALL
 ****************************************************
 ******************* SOLVE FOR LS 1 OF 1 ****************

 SELECT       FOR ITEM=TYPE COMPONENT=    
  IN RANGE        45 TO         45 STEP          1

        826  ELEMENTS (OF      29307  DEFINED) SELECTED BY  ESEL  COMMAND.

 SELECT      ALL NODES HAVING ANY ELEMENT IN ELEMENT SET.

     1688 NODES (OF    77114  DEFINED) SELECTED FROM
      826 SELECTED ELEMENTS BY NSLE COMMAND.

 SPECIFIED SURFACE LOAD PRES FOR ALL SELECTED ELEMENTS  LKEY =  1   KVAL = 1
      SET ACCORDING TO TABLE PARAMETER = _LOADVARI106X                   

 SPECIFIED SURFACE LOAD PRES FOR ALL SELECTED ELEMENTS  LKEY =  2   KVAL = 1
      SET ACCORDING TO TABLE PARAMETER = _LOADVARI106Y                   

 SPECIFIED SURFACE LOAD PRES FOR ALL SELECTED ELEMENTS  LKEY =  3   KVAL = 1
      SET ACCORDING TO TABLE PARAMETER = _LOADVARI106Z                   

 ALL SELECT   FOR ITEM=NODE COMPONENT=    
  IN RANGE         1 TO      77114 STEP          1

      77114  NODES (OF      77114  DEFINED) SELECTED BY NSEL  COMMAND.

 ALL SELECT   FOR ITEM=ELEM COMPONENT=    
  IN RANGE         1 TO      29307 STEP          1

      29307  ELEMENTS (OF      29307  DEFINED) SELECTED BY  ESEL  COMMAND.

 PRINTOUT RESUMED BY /GOP

 DO NOT USE AUTOMATIC TIME STEPPING THIS LOAD STEP

 USE       1 SUBSTEPS INITIALLY THIS LOAD STEP FOR ALL  DEGREES OF FREEDOM
 FOR AUTOMATIC TIME STEPPING:
   USE      1 SUBSTEPS AS A MAXIMUM
   USE      1 SUBSTEPS AS A MINIMUM

 TIME=  1.0000    

 ERASE THE CURRENT DATABASE OUTPUT CONTROL TABLE.


 WRITE ALL  ITEMS TO THE DATABASE WITH A FREQUENCY OF NONE
   FOR ALL APPLICABLE ENTITIES

 WRITE NSOL ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 WRITE RSOL ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 WRITE STRS ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 WRITE EPEL ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 WRITE EPPL ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 NONLINEAR STABILIZATION CONTROL:
 KEY=OFF 


 *GET  ANSINTER_  FROM  ACTI  ITEM=INT        VALUE=  0.00000000    

 *IF  ANSINTER_                         ( =   0.00000     )  NE  
      0                                 ( =   0.00000     )  THEN    

 *ENDIF

 *****  ANSYS SOLVE    COMMAND  *****

 *** WARNING ***                         CP =       0.844   TIME= 18:56:33
 Element shape checking is currently inactive.  Issue SHPP,ON or         
 SHPP,WARN to reactivate, if desired.                                    

 *** NOTE ***                            CP =       0.906   TIME= 18:56:33
 The model data was checked and warning messages were found.             
  Please review output or errors file (                                  
 C:\Users\azer.b\AppData\Local\Temp\WB_OLEG-WS_Oleg.g_5632_2\_ProjectScr 
 ratch\ScrC268\file0.err ) for these warning messages.                   

 *** SELECTION OF ELEMENT TECHNOLOGIES FOR APPLICABLE ELEMENTS ***
      --- GIVE SUGGESTIONS AND RESET THE KEY OPTIONS ---

 ELEMENT TYPE    1 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE    2 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE    3 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE    4 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE    5 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE    6 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE    7 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE    8 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE    9 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   10 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.



 *** ANSYS - ENGINEERING ANALYSIS SYSTEM  RELEASE Release 18.1     18.1     ***
 DISTRIBUTED ANSYS Multiphysics                                

 00000000  VERSION=WINDOWS x64   18:56:33  SEP 12, 2017 CP=      0.938

 unsaved_project--Static Structural (C5)                                       



                       S O L U T I O N   O P T I O N S

   PROBLEM DIMENSIONALITY. . . . . . . . . . . . .3-D                  
   DEGREES OF FREEDOM. . . . . . UX   UY   UZ  
   ANALYSIS TYPE . . . . . . . . . . . . . . . . .STATIC (STEADY-STATE)
   OFFSET TEMPERATURE FROM ABSOLUTE ZERO . . . . .  273.15    
   EQUATION SOLVER OPTION. . . . . . . . . . . . .SPARSE             
   NEWTON-RAPHSON OPTION . . . . . . . . . . . . .PROGRAM CHOSEN   
   GLOBALLY ASSEMBLED MATRIX . . . . . . . . . . .SYMMETRIC  

 *** WARNING ***                         CP =       1.031   TIME= 18:56:33
 Material number 45 (used by element 28482 ) should normally have at     
 least one MP or one TB type command associated with it.  Output of      
 energy by material may not be available.                                

 *** NOTE ***                            CP =       1.062   TIME= 18:56:33
 The step data was checked and warning messages were found.              
  Please review output or errors file (                                  
 C:\Users\azer.b\AppData\Local\Temp\WB_OLEG-WS_Oleg.g_5632_2\_ProjectScr 
 ratch\ScrC268\file0.err ) for these warning messages.                   

 *** NOTE ***                            CP =       1.062   TIME= 18:56:33
 This nonlinear analysis defaults to using the full Newton-Raphson       
 solution procedure.  This can be modified using the NROPT command.      

 *** NOTE ***                            CP =       1.062   TIME= 18:56:33
 The conditions for direct assembly have been met.  No .emat or .erot    
 files will be produced.                                                 

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 11 and contact element type 11 has been set up.  The       
 companion pair has real constant set ID 12.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.41737E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49689E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.9379    
 Average contact pair depth                    10.000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5000    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Max.  Initial penetration 7.105427358E-15 was detected between contact  
 element 21053 and target element 21748.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 12 and contact element type 11 has been set up.  The       
 companion pair has real constant set ID 11.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.41737E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0063    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.48798E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.7596    
 Average contact pair depth                    10.063    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5157    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Max.  Initial penetration 7.105427358E-15 was detected between contact  
 element 21523 and target element 20826.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 13 and contact element type 13 has been set up.  The       
 companion pair has real constant set ID 14.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.42000E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50114E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.023    
 Average contact pair depth                    10.000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5000    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 21964 and target element 22044.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 14 and contact element type 13 has been set up.  The       
 companion pair has real constant set ID 13.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.42000E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.96205    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    9.6205    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.4051    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22016 and target element 21916.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 15 and contact element type 15 has been set up.  The       
 companion pair has real constant set ID 16.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.37663E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49651E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.9303    
 Average contact pair depth                    10.000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5000    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22124 and target element 22192.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 16 and contact element type 15 has been set up.  The       
 companion pair has real constant set ID 15.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.37663E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.1152    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    11.152    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.7879    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22166 and target element 22078.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.812   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 17 and contact element type 17 has been set up.  The       
 companion pair has real constant set ID 18.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.42000E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50001E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    10.000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5000    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22286 and target element 22347.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 18 and contact element type 17 has been set up.  The       
 companion pair has real constant set ID 17.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.42000E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.97498    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    9.7498    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.4374    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22323 and target element 22237.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 19 and contact element type 19 has been set up.  The       
 companion pair has real constant set ID 20.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.36951E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49993E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.9986    
 Average contact pair depth                    10.000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5000    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22418 and target element 22492.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 20 and contact element type 19 has been set up.  The       
 companion pair has real constant set ID 19.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.36951E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.1367    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    11.367    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.8416    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22450 and target element 22364.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 21 and contact element type 21 has been set up.  The       
 companion pair has real constant set ID 22.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46667E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49496E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.8993    
 Average contact pair depth                    9.0000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2500    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 22703 and target element 23072.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 22 and contact element type 21 has been set up.  The       
 companion pair has real constant set ID 21.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46667E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.61177    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49314E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.8629    
 Average contact pair depth                    6.1177    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  1.5294    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 9.094947018E-13 was detected between contact  
 element 22952 and target element 22572.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 23 and contact element type 23 has been set up.  The       
 companion pair has real constant set ID 24.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46667E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50149E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.030    
 Average contact pair depth                    9.0000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2500    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 23361 and target element 23715.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 24 and contact element type 23 has been set up.  The       
 companion pair has real constant set ID 23.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46667E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.60932    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50648E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.130    
 Average contact pair depth                    6.0932    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  1.5233    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 23562 and target element 23185.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 25 and contact element type 25 has been set up.  The       
 companion pair has real constant set ID 26.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.44651E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.48518E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.7036    
 Average contact pair depth                    9.0000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2500    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 23854 and target element 23917.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 26 and contact element type 25 has been set up.  The       
 companion pair has real constant set ID 25.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.44651E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.94064    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    9.4064    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.3516    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 23894 and target element 23838.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 27 and contact element type 27 has been set up.  The       
 companion pair has real constant set ID 28.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.43109E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.48753E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.7506    
 Average contact pair depth                    9.0000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2500    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 23970 and target element 24037.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 28 and contact element type 27 has been set up.  The       
 companion pair has real constant set ID 27.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.43109E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.97427    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    9.7427    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.4357    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 24018 and target element 23943.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 29 and contact element type 29 has been set up.  The       
 companion pair has real constant set ID 30.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.45472E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.48166E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.6333    
 Average contact pair depth                    9.0000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2500    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 24093 and target element 24155.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 30 and contact element type 29 has been set up.  The       
 companion pair has real constant set ID 29.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.45472E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.92364    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    9.2364    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.3091    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 24136 and target element 24058.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 31 and contact element type 31 has been set up.  The       
 companion pair has real constant set ID 32.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.43816E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.48406E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.6813    
 Average contact pair depth                    9.0000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2500    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 24213 and target element 24282.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 32 and contact element type 31 has been set up.  The       
 companion pair has real constant set ID 31.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.43816E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.95856    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    9.5856    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.3964    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 24256 and target element 24192.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 33 and contact element type 33 has been set up.  The       
 companion pair has real constant set ID 34.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.45874E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.73263    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.46103E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.2206    
 Average contact pair depth                    7.3263    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  1.8316    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Min.  Initial gap 2.682163205E-02 was detected between contact element  
 24334 and target element 24514.                                         
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 0.875715412 has been detected between contact       
 element 24340 and target element 24517.                                 
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 34 and contact element type 33 has been set up.  The       
 companion pair has real constant set ID 33.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.45874E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.91555    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.55365E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                11.073    
 Average contact pair depth                    9.1555    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2889    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Min.  Initial gap 1.036004433E-03 was detected between contact element  
 24392 and target element 24303.                                         
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 3.73976654 has been detected between contact        
 element 24421 and target element 24295.                                 
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 35 and contact element type 35 has been set up.  The       
 companion pair has real constant set ID 36.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.44989E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35773    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49172E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.8344    
 Average contact pair depth                    3.5773    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.89433    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 36 and contact element type 35 has been set up.  The       
 companion pair has real constant set ID 35.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.44989E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.93356    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.54680E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.936    
 Average contact pair depth                    9.3356    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.3339    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Min.  Initial gap 1.2500685 was detected between contact element 24702  
 and target element 24595.                                               
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 3.04307023 has been detected between contact        
 element 24748 and target element 24590.                                 
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 37 and contact element type 37 has been set up.  The       
 companion pair has real constant set ID 38.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.40632E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0337    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.37965E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                7.5929    
 Average contact pair depth                    10.337    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5842    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Min.  Initial gap 8.85567474E-04 was detected between contact element   
 24913 and target element 25058.                                         
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 2.26769275 has been detected between contact        
 element 24919 and target element 25057.                                 
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 38 and contact element type 37 has been set up.  The       
 companion pair has real constant set ID 37.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.40632E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.96778    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.53652E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.730    
 Average contact pair depth                    9.6778    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.4194    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Min.  Initial gap 2.134222638E-03 was detected between contact element  
 24948 and target element 24888.                                         
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 2.89613004 has been detected between contact        
 element 24982 and target element 24880.                                 
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 39 and contact element type 39 has been set up.  The       
 companion pair has real constant set ID 40.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46525E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36764    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.48682E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.7364    
 Average contact pair depth                    3.6764    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.91911    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 40 and contact element type 39 has been set up.  The       
 companion pair has real constant set ID 39.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46525E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90273    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.55109E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                11.022    
 Average contact pair depth                    9.0273    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2568    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Min.  Initial gap 1.235717 was detected between contact element 25263   
 and target element 25123.                                               
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 2.89639326 has been detected between contact        
 element 25283 and target element 25120.                                 
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 41 and contact element type 41 has been set up.  The       
 companion pair has real constant set ID 42.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.40660E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0330    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.37965E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                7.5929    
 Average contact pair depth                    10.330    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5824    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Min.  Initial gap 7.340451554E-04 was detected between contact element  
 25435 and target element 25587.                                         
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 2.10699742 has been detected between contact        
 element 25428 and target element 25563.                                 
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 42 and contact element type 41 has been set up.  The       
 companion pair has real constant set ID 41.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.40660E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.92461    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.52189E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.438    
 Average contact pair depth                    9.2461    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.3115    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 1.046756503E-05 was detected between contact  
 element 25516 and target element 25408.                                 
 You may move entire target surface by : x= 3.181284813E-08, y=          
 7.72621808E-11, z= 1.046751669E-05,to reduce initial penetration.       
  
 Max.  Geometric gap 2.98724196 has been detected between contact        
 element 25509 and target element 25417.                                 
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 43 and contact element type 43 has been set up.  The       
 companion pair has real constant set ID 44.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.44647E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.91784    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.56996E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                11.399    
 Average contact pair depth                    9.1784    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2946    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 1.383818148E-02 was detected between contact  
 element 26562 and target element 28390.                                 
 You may move entire target surface by : x= 2.330569966E-04, y=          
 1.383588889E-02, z= 9.554943146E-05,to reduce initial penetration.      
  
 Max.  Geometric gap 2.72655074 has been detected between contact        
 element 26590 and target element 28392.                                 
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 44 and contact element type 43 has been set up.  The       
 companion pair has real constant set ID 43.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.44647E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.94072    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.53551E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.710    
 Average contact pair depth                    9.4072    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.3518    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       1.844   TIME= 18:56:34
 Max.  Initial penetration 1.749607542E-02 was detected between contact  
 element 27787 and target element 26012.                                 
 You may move entire target surface by : x= 3.226562824E-16, y=          
 1.749607542E-02, z= -7.576086216E-16,to reduce initial penetration.     
  
 Max.  Geometric gap 2.20998935 has been detected between contact        
 element 27777 and target element 26118.                                 
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  
  
  

  
  
     D I S T R I B U T E D   D O M A I N   D E C O M P O S E R
  
  ...Number of elements: 29307
  ...Number of nodes:    77114
  ...Decompose to 2 CPU domains
  ...Element load balance ratio =     1.024


                      L O A D   S T E P   O P T I O N S

   LOAD STEP NUMBER. . . . . . . . . . . . . . . .     1
   TIME AT END OF THE LOAD STEP. . . . . . . . . .  1.0000    
   NUMBER OF SUBSTEPS. . . . . . . . . . . . . . .     1
   MAXIMUM NUMBER OF EQUILIBRIUM ITERATIONS. . . .     1
   STEP CHANGE BOUNDARY CONDITIONS . . . . . . . .    NO
   TERMINATE ANALYSIS IF NOT CONVERGED . . . . . .YES (EXIT)  
   CONVERGENCE CONTROLS. . . . . . . . . . . . . .USE DEFAULTS
   PRINT OUTPUT CONTROLS . . . . . . . . . . . . .NO PRINTOUT
   DATABASE OUTPUT CONTROLS
      ITEM     FREQUENCY   COMPONENT
       ALL       NONE               
      NSOL        ALL               
      RSOL        ALL               
      STRS        ALL               
      EPEL        ALL               
      EPPL        ALL               


 SOLUTION MONITORING INFO IS WRITTEN TO FILE= file.mntr                                                                                                                                                                                                                                                           

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 11 and contact element type 11 has been set up.  The       
 companion pair has real constant set ID 12.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.41737E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49689E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.9379    
 Average contact pair depth                    10.000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5000    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 7.105427358E-15 was detected between contact  
 element 21053 and target element 21748.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 12 and contact element type 11 has been set up.  The       
 companion pair has real constant set ID 11.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.41737E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0063    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.48798E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.7596    
 Average contact pair depth                    10.063    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5157    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 7.105427358E-15 was detected between contact  
 element 21523 and target element 20826.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 15 and contact element type 15 has been set up.  The       
 companion pair has real constant set ID 16.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.37663E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49651E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.9303    
 Average contact pair depth                    10.000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5000    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22124 and target element 22192.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 16 and contact element type 15 has been set up.  The       
 companion pair has real constant set ID 15.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.37663E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.1152    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    11.152    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.7879    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22166 and target element 22078.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 19 and contact element type 19 has been set up.  The       
 companion pair has real constant set ID 20.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.36951E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49993E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.9986    
 Average contact pair depth                    10.000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5000    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22418 and target element 22492.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 20 and contact element type 19 has been set up.  The       
 companion pair has real constant set ID 19.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.36951E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.1367    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    11.367    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.8416    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 22450 and target element 22364.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 21 and contact element type 21 has been set up.  The       
 companion pair has real constant set ID 22.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46667E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49496E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.8993    
 Average contact pair depth                    9.0000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2500    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 22703 and target element 23072.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 22 and contact element type 21 has been set up.  The       
 companion pair has real constant set ID 21.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46667E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.61177    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.49314E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.8629    
 Average contact pair depth                    6.1177    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  1.5294    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 9.094947018E-13 was detected between contact  
 element 22952 and target element 22572.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 23 and contact element type 23 has been set up.  The       
 companion pair has real constant set ID 24.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46667E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50149E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.030    
 Average contact pair depth                    9.0000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2500    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 23361 and target element 23715.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 24 and contact element type 23 has been set up.  The       
 companion pair has real constant set ID 23.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46667E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.60932    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50648E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.130    
 Average contact pair depth                    6.0932    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  1.5233    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 23562 and target element 23185.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 25 and contact element type 25 has been set up.  The       
 companion pair has real constant set ID 26.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.44651E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.48518E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.7036    
 Average contact pair depth                    9.0000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2500    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 23854 and target element 23917.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 26 and contact element type 25 has been set up.  The       
 companion pair has real constant set ID 25.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.44651E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.94064    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    9.4064    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.3516    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 23894 and target element 23838.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 27 and contact element type 27 has been set up.  The       
 companion pair has real constant set ID 28.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.43109E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90000    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.48753E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.7506    
 Average contact pair depth                    9.0000    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2500    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 23970 and target element 24037.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 28 and contact element type 27 has been set up.  The       
 companion pair has real constant set ID 27.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.43109E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.97427    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.50000E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.000    
 Average contact pair depth                    9.7427    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.4357    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Max.  Initial penetration 4.547473509E-13 was detected between contact  
 element 24018 and target element 23943.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 33 and contact element type 33 has been set up.  The       
 companion pair has real constant set ID 34.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.45874E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.73263    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.46103E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.2206    
 Average contact pair depth                    7.3263    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  1.8316    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Min.  Initial gap 2.682163205E-02 was detected between contact element  
 24334 and target element 24514.                                         
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 0.875715412 has been detected between contact       
 element 24340 and target element 24517.                                 
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 34 and contact element type 33 has been set up.  The       
 companion pair has real constant set ID 33.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.45874E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.91555    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.55365E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                11.073    
 Average contact pair depth                    9.1555    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2889    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Min.  Initial gap 1.036004433E-03 was detected between contact element  
 24392 and target element 24303.                                         
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 3.73976654 has been detected between contact        
 element 24421 and target element 24295.                                 
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 37 and contact element type 37 has been set up.  The       
 companion pair has real constant set ID 38.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.40632E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance           1.0337    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.37965E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                7.5929    
 Average contact pair depth                    10.337    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.5842    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Min.  Initial gap 8.85567474E-04 was detected between contact element   
 24913 and target element 25058.                                         
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 2.26769275 has been detected between contact        
 element 24919 and target element 25057.                                 
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 38 and contact element type 37 has been set up.  The       
 companion pair has real constant set ID 37.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.40632E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.96778    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.53652E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                10.730    
 Average contact pair depth                    9.6778    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.4194    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Min.  Initial gap 2.134222638E-03 was detected between contact element  
 24948 and target element 24888.                                         
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 2.89613004 has been detected between contact        
 element 24982 and target element 24880.                                 
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 39 and contact element type 39 has been set up.  The       
 companion pair has real constant set ID 40.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46525E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36764    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.48682E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                9.7364    
 Average contact pair depth                    3.6764    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.91911    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 40 and contact element type 39 has been set up.  The       
 companion pair has real constant set ID 39.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.46525E+07
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.90273    
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip tolerance         0.55109E-01
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length                11.022    
 Average contact pair depth                    9.0273    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                  2.2568    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =       2.969   TIME= 18:56:34
 Min.  Initial gap 1.235717 was detected between contact element 25263   
 and target element 25123.                                               
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 2.89639326 has been detected between contact        
 element 25283 and target element 25120.                                 
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          11

 *** NOTE ***                            CP =       4.703   TIME= 18:56:36
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          12
 Max.  Penetration of 0 has been detected between contact element 21418  
 and target element 21021.                                               
  
 Max.  Geometrical gap of 7.105427358E-15 has been detected between      
 contact element 21434 and target element 20663.                         
  
 Max.  Geometrical penetration of -7.105427358E-15 has been detected     
 between contact element 21434 and target element 20663.                 
 For total 244 contact elements, there are 244 elements are in contact.  
 There are 244 elements are in sticking.                                 
 Contacting area 21960.                                                  
 Max.  Pinball distance 2.51574693.                                      
 One of the contact searching regions contains at least 30 target        
 elements.                                                               
 Max.  Pressure/force 3.617887493E-08.                                   
 Max.  Normal stiffness 4173710.75.                                      
 Min.  Normal stiffness 4173710.75.                                      
 Max.  Tangential stiffness 3227587.77.                                  
 Min.  Tangential stiffness 3227587.77.                                  
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          15

 *** NOTE ***                            CP =       4.703   TIME= 18:56:36
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          16
 Max.  Penetration of 0 has been detected between contact element 22166  
 and target element 22075.                                               
  
 Max.  Geometrical gap of 3.552713679E-15 has been detected between      
 contact element 22169 and target element 22085.                         
  
 Max.  Geometrical penetration of -3.552713679E-15 has been detected     
 between contact element 22169 and target element 22085.                 
 For total 26 contact elements, there are 26 elements are in contact.    
 There are 26 elements are in sticking.                                  
 Contacting area 2600.                                                   
 Max.  Pinball distance 2.78789217.                                      
 One of the contact searching regions contains at least 12 target        
 elements.                                                               
 Max.  Pressure/force 3.345134187E-08.                                   
 Max.  Normal stiffness 3766286.27.                                      
 Min.  Normal stiffness 3766286.27.                                      
 Max.  Tangential stiffness 3150000.                                     
 Min.  Tangential stiffness 3150000.                                     
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          19

 *** NOTE ***                            CP =       4.703   TIME= 18:56:36
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          20
 Max.  Penetration of 0 has been detected between contact element 22450  
 and target element 22364.                                               
  
 Max.  Geometrical gap of 7.105427358E-15 has been detected between      
 contact element 22453 and target element 22373.                         
  
 Max.  Geometrical penetration of -3.552713679E-15 has been detected     
 between contact element 22453 and target element 22373.                 
 For total 26 contact elements, there are 26 elements are in contact.    
 There are 26 elements are in sticking.                                  
 Contacting area 2600.                                                   
 Max.  Pinball distance 2.84163518.                                      
 One of the contact searching regions contains at least 15 target        
 elements.                                                               
 Max.  Pressure/force 3.281868649E-08.                                   
 Max.  Normal stiffness 3695055.61.                                      
 Min.  Normal stiffness 3695055.61.                                      
 Max.  Tangential stiffness 3150000.                                     
 Min.  Tangential stiffness 3150000.                                     
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          21

 *** NOTE ***                            CP =       4.703   TIME= 18:56:36
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          22
 Max.  Penetration of 0 has been detected between contact element 22904  
 and target element 22604.                                               
  
 Max.  Geometrical gap of 4.547473509E-13 has been detected between      
 contact element 22952 and target element 22572.                         
  
 Max.  Geometrical penetration of -9.094947018E-13 has been detected     
 between contact element 22952 and target element 22572.                 
 For total 128 contact elements, there are 128 elements are in contact.  
 There are 128 elements are in sticking.                                 
 Contacting area 12063.7335.                                             
 Max.  Pinball distance 1.52943066.                                      
 One of the contact searching regions contains at least 11 target        
 elements.                                                               
 Max.  Pressure/force 4.087998208E-08.                                   
 Max.  Normal stiffness 4666666.67.                                      
 Min.  Normal stiffness 4666666.67.                                      
 Max.  Tangential stiffness 2170971.54.                                  
 Min.  Tangential stiffness 2170971.54.                                  
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          23

 *** NOTE ***                            CP =       4.703   TIME= 18:56:36
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          24
 Max.  Penetration of 0 has been detected between contact element 23562  
 and target element 23185.                                               
  
 Max.  Geometrical gap of 4.547473509E-13 has been detected between      
 contact element 23562 and target element 23185.                         
  
 Max.  Geometrical penetration of -4.547473509E-13 has been detected     
 between contact element 23562 and target element 23185.                 
 For total 121 contact elements, there are 121 elements are in contact.  
 There are 121 elements are in sticking.                                 
 Contacting area 12063.7335.                                             
 Max.  Pinball distance 1.52329074.                                      
 One of the contact searching regions contains at least 13 target        
 elements.                                                               
 Max.  Pressure/force 4.198578565E-08.                                   
 Max.  Normal stiffness 4666666.67.                                      
 Min.  Normal stiffness 4666666.67.                                      
 Max.  Tangential stiffness 2105307.57.                                  
 Min.  Tangential stiffness 2105307.57.                                  
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          25

 *** NOTE ***                            CP =       4.703   TIME= 18:56:36
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          26
 Max.  Penetration of 0 has been detected between contact element 23894  
 and target element 23835.                                               
  
 Max.  Geometrical gap of 4.547473509E-13 has been detected between      
 contact element 23894 and target element 23838.                         
  
 Max.  Geometrical penetration of -4.547473509E-13 has been detected     
 between contact element 23894 and target element 23838.                 
 For total 16 contact elements, there are 16 elements are in contact.    
 There are 16 elements are in sticking.                                  
 Contacting area 1600.                                                   
 Max.  Pinball distance 2.35158845.                                      
 One of the contact searching regions contains at least 18 target        
 elements.                                                               
 Max.  Pressure/force 3.965776165E-08.                                   
 Max.  Normal stiffness 4465067.01.                                      
 Min.  Normal stiffness 4465067.01.                                      
 Max.  Tangential stiffness 3150000.                                     
 Min.  Tangential stiffness 3150000.                                     
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          27

 *** NOTE ***                            CP =       4.703   TIME= 18:56:36
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          28
 Max.  Penetration of 0 has been detected between contact element 24014  
 and target element 23959.                                               
  
 Max.  Geometrical gap of 4.547473509E-13 has been detected between      
 contact element 24014 and target element 23959.                         
  
 Max.  Geometrical penetration of -4.547473509E-13 has been detected     
 between contact element 24014 and target element 23959.                 
 For total 16 contact elements, there are 16 elements are in contact.    
 There are 16 elements are in sticking.                                  
 Contacting area 1600.                                                   
 Max.  Pinball distance 2.43567621.                                      
 One of the contact searching regions contains at least 14 target        
 elements.                                                               
 Max.  Pressure/force 3.828864188E-08.                                   
 Max.  Normal stiffness 4310917.83.                                      
 Min.  Normal stiffness 4310917.83.                                      
 Max.  Tangential stiffness 3150000.                                     
 Min.  Tangential stiffness 3150000.                                     
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          33
 Max.  Penetration of -2.84537269E-14 has been detected between contact  
 element 24334 and target element 24527.                                 
  
 Max.  Geometrical gap of 0.875715412 has been detected between contact  
 element 24340 and target element 24517.                                 
 For total 32 contact elements, there are 16 elements are in contact.    
 There are 16 elements are in sticking.                                  
 Contacting area 1066.34537.                                             
 Max.  Pinball distance 1.83158193.                                      
 One of the contact searching regions contains at least 14 target        
 elements.                                                               
 Max.  Pressure/force -2.707037421E-07.                                  
 Max.  Normal stiffness 4587388.57.                                      
 Min.  Normal stiffness 4587388.57.                                      
 Max.  Tangential stiffness 2733714.4.                                   
 Min.  Tangential stiffness 2733714.4.                                   
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          34

 *** NOTE ***                            CP =       4.703   TIME= 18:56:36
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          37
 Max.  Penetration of -3.007744142E-14 has been detected between contact 
 element 24910 and target element 25052.                                 
  
 Max.  Geometrical gap of 2.26769275 has been detected between contact   
 element 24919 and target element 25057.                                 
 *WARNING*: The geometrical gap may be too large.  Increase pinball if   
 it is a true geometrical gap.  Decrease pinball if it is a false one.   
 For total 27 contact elements, there are 15 elements are in contact.    
 There are 15 elements are in sticking.                                  
 Contacting area 879.428609.                                             
 Max.  Pinball distance 2.58418049.                                      
 One of the contact searching regions contains at least 12 target        
 elements.                                                               
 Max.  Pressure/force -4.860947152E-07.                                  
 Max.  Normal stiffness 4063183.68.                                      
 Min.  Normal stiffness 4063183.68.                                      
 Max.  Tangential stiffness 4148612.34.                                  
 Min.  Tangential stiffness 4148612.34.                                  
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          38

 *** NOTE ***                            CP =       4.703   TIME= 18:56:36
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          39

 *** NOTE ***                            CP =       4.703   TIME= 18:56:36
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          40
 Max.  Penetration of -9.120957883E-13 has been detected between contact 
 element 25216 and target element 25124.                                 
  
 Max.  Geometrical gap of 2.23497684 has been detected between contact   
 element 25242 and target element 25085.                                 
 *WARNING*: The geometrical gap may be too large.  Increase pinball if   
 it is a true geometrical gap.  Decrease pinball if it is a false one.   
 For total 90 contact elements, there are 31 elements are in contact.    
 There are 31 elements are in sticking.                                  
 Contacting area 830.821735.                                             
 Max.  Pinball distance 2.25683326.                                      
 One of the contact searching regions contains at least 12 target        
 elements.                                                               
 Max.  Pressure/force -4.352384557E-06.                                  
 Max.  Normal stiffness 4652536.88.                                      
 Min.  Normal stiffness 4652536.88.                                      
 Max.  Tangential stiffness 2857976.02.                                  
 Min.  Tangential stiffness 2857976.02.                                  
 *************************************************


                         ***********  PRECISE MASS SUMMARY  ***********

   TOTAL RIGID BODY MASS MATRIX ABOUT ORIGIN
               Translational mass               |   Coupled translational/rotational mass
        0.98662E-01    0.0000        0.0000     |     0.0000        9.9077       -237.55    
         0.0000       0.98662E-01    0.0000     |    -9.9077        0.0000        61.630    
         0.0000        0.0000       0.98662E-01 |     237.55       -61.630        0.0000    
     ------------------------------------------ | ------------------------------------------
                                                |         Rotational mass (inertia)
                                                |    0.57494E+06  -0.14840E+06   -6704.0    
                                                |   -0.14840E+06    42965.       -23866.    
                                                |    -6704.0       -23866.       0.61351E+06

   TOTAL MASS = 0.98662E-01
     The mass principal axes coincide with the global Cartesian axes

   CENTER OF MASS (X,Y,Z)=    624.66        2407.7        100.42    

   TOTAL INERTIA ABOUT CENTER OF MASS
         1982.9       -7.4423       -515.03    
        -7.4423        3472.2       -10.744    
        -515.03       -10.744        3040.2    

   PRINCIPAL INERTIAS =    1773.4        3472.5        3249.4    
   ORIENTATION VECTORS OF THE INERTIA PRINCIPAL AXES IN GLOBAL CARTESIAN
     ( 0.926, 0.006, 0.377) ( 0.006, 0.999,-0.032) (-0.377, 0.032, 0.926) 


  *** MASS SUMMARY BY ELEMENT TYPE ***

  TYPE      MASS
     1  0.404831E-01
     2  0.219053E-01
     3  0.208094E-02
     4  0.208094E-02
     5  0.148928E-02
     6  0.148928E-02
     7  0.148928E-02
     8  0.148928E-02
     9  0.181447E-01
    10  0.800966E-02

 Range of element maximum matrix coefficients in global coordinates
 Maximum = 189123762 at element 22949.                                   
 Minimum = 296213.893 at element 11826.                                  

   *** ELEMENT MATRIX FORMULATION TIMES
     TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

        1      5360  SOLID186      0.734   0.000137
        2      3248  SOLID186      0.422   0.000130
        3       512  SOLID186      0.141   0.000275
        4       484  SOLID186      0.031   0.000065
        5       228  SOLID186      0.031   0.000137
        6       214  SOLID186      0.031   0.000146
        7       232  SOLID186      0.031   0.000135
        8       206  SOLID186      0.031   0.000152
        9      6328  SOLID187      0.391   0.000062
       10      3839  SOLID187      0.281   0.000073
       11       627  CONTA174      0.000   0.000000
       12       627  TARGE170      0.016   0.000025
       13        81  CONTA174      0.000   0.000000
       14        81  TARGE170      0.000   0.000000
       15        75  CONTA174      0.000   0.000000
       16        75  TARGE170      0.000   0.000000
       17        71  CONTA174      0.000   0.000000
       18        71  TARGE170      0.016   0.000220
       19        71  CONTA174      0.000   0.000000
       20        71  TARGE170      0.000   0.000000
       21       329  CONTA174      0.047   0.000142
       22       329  TARGE170      0.016   0.000047
       23       322  CONTA174      0.031   0.000097
       24       322  TARGE170      0.000   0.000000
       25        61  CONTA174      0.000   0.000000
       26        61  TARGE170      0.000   0.000000
       27        60  CONTA174      0.000   0.000000
       28        60  TARGE170      0.000   0.000000
       29        61  CONTA174      0.016   0.000256
       30        61  TARGE170      0.000   0.000000
       31        60  CONTA174      0.000   0.000000
       32        60  TARGE170      0.000   0.000000
       33       127  CONTA174      0.016   0.000123
       34       127  TARGE170      0.000   0.000000
       35       166  CONTA174      0.000   0.000000
       36       166  TARGE170      0.000   0.000000
       37       105  CONTA174      0.000   0.000000
       38       105  TARGE170      0.000   0.000000
       39       155  CONTA174      0.000   0.000000
       40       155  TARGE170      0.000   0.000000
       41       107  CONTA174      0.000   0.000000
       42       107  TARGE170      0.000   0.000000
       43      1437  CONTA174      0.062   0.000043
       44      1437  TARGE170      0.016   0.000011
       45       826  SURF154       0.078   0.000095
 Time at end of element matrix formulation CP = 4.703125.                
     FORCE CONVERGENCE VALUE  =   7347.      CRITERION=   37.49    

 DISTRIBUTED SPARSE MATRIX DIRECT SOLVER.
  Number of equations =      230130,    Maximum wavefront =    321

 *** NOTE ***                            CP =       6.156   TIME= 18:56:38
 The initial memory allocation (-m) has been exceeded.                   
  Supplemental memory allocations are being used.                        

  Local memory allocated for solver              =   1081.905 MB
  Local memory required for in-core solution     =    958.039 MB
  Local memory required for out-of-core solution =    362.889 MB

  Total memory allocated for solver              =   2072.514 MB
  Total memory required for in-core solution     =   1828.495 MB
  Total memory required for out-of-core solution =    636.563 MB

 *** NOTE ***                            CP =       6.156   TIME= 18:56:38
 The Distributed Sparse Matrix Solver is currently running in the        
 in-core memory mode.  This memory mode uses the most amount of memory   
 in order to avoid using the hard drive as much as possible, which most  
 often results in the fastest solution time.  This mode is recommended   
 if enough physical memory is present to accommodate all of the solver   
 data.                                                                   
 curEqn=  91515  totEqn= 129000 Job CP sec=     10.375
      Factor Done=  50% Factor Wall sec=      3.379 rate=   17359.6 Mflops
 curEqn= 129000  totEqn= 129000 Job CP sec=     13.906
      Factor Done= 100% Factor Wall sec=      6.922 rate=   16940.0 Mflops
 Distributed sparse solver maximum pivot= 182292929 at node 32265 UY.    
 Distributed sparse solver minimum pivot= 9432.78752 at node 11613 UX.   
 Distributed sparse solver minimum pivot in absolute value= 9432.78752   
 at node 11613 UX.                                                       
     DISP CONVERGENCE VALUE   =  0.2350      CRITERION=  0.1199E-01

   *** ELEMENT RESULT CALCULATION TIMES
     TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

        1      5360  SOLID186      0.422   0.000079
        2      3248  SOLID186      0.250   0.000077
        3       512  SOLID186      0.047   0.000092
        4       484  SOLID186      0.016   0.000032
        5       228  SOLID186      0.000   0.000000
        6       214  SOLID186      0.031   0.000146
        7       232  SOLID186      0.031   0.000135
        8       206  SOLID186      0.016   0.000076
        9      6328  SOLID187      0.312   0.000049
       10      3839  SOLID187      0.203   0.000053
       11       627  CONTA174      0.000   0.000000
       13        81  CONTA174      0.000   0.000000
       15        75  CONTA174      0.000   0.000000
       17        71  CONTA174      0.016   0.000220
       19        71  CONTA174      0.000   0.000000
       21       329  CONTA174      0.000   0.000000
       23       322  CONTA174      0.031   0.000097
       25        61  CONTA174      0.000   0.000000
       27        60  CONTA174      0.000   0.000000
       29        61  CONTA174      0.000   0.000000
       31        60  CONTA174      0.000   0.000000
       33       127  CONTA174      0.000   0.000000
       35       166  CONTA174      0.000   0.000000
       37       105  CONTA174      0.000   0.000000
       39       155  CONTA174      0.000   0.000000
       41       107  CONTA174      0.000   0.000000
       43      1437  CONTA174      0.031   0.000022
       45       826  SURF154       0.031   0.000038

   *** NODAL LOAD CALCULATION TIMES
     TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

        1      5360  SOLID186      0.031   0.000006
        2      3248  SOLID186      0.000   0.000000
        3       512  SOLID186      0.000   0.000000
        4       484  SOLID186      0.000   0.000000
        5       228  SOLID186      0.000   0.000000
        6       214  SOLID186      0.000   0.000000
        7       232  SOLID186      0.000   0.000000
        8       206  SOLID186      0.000   0.000000
        9      6328  SOLID187      0.016   0.000002
       10      3839  SOLID187      0.016   0.000004
       11       627  CONTA174      0.000   0.000000
       13        81  CONTA174      0.000   0.000000
       15        75  CONTA174      0.000   0.000000
       17        71  CONTA174      0.000   0.000000
       19        71  CONTA174      0.000   0.000000
       21       329  CONTA174      0.000   0.000000
       23       322  CONTA174      0.000   0.000000
       25        61  CONTA174      0.000   0.000000
       27        60  CONTA174      0.000   0.000000
       29        61  CONTA174      0.000   0.000000
       31        60  CONTA174      0.000   0.000000
       33       127  CONTA174      0.000   0.000000
       35       166  CONTA174      0.000   0.000000
       37       105  CONTA174      0.000   0.000000
       39       155  CONTA174      0.000   0.000000
       41       107  CONTA174      0.000   0.000000
       43      1437  CONTA174      0.016   0.000011
       45       826  SURF154       0.016   0.000019
 *** LOAD STEP     1   SUBSTEP     1  COMPLETED.    CUM ITER =      1
 *** TIME =   1.00000         TIME INC =   1.00000      NEW TRIANG MATRIX


 *** ANSYS BINARY FILE STATISTICS
  BUFFER SIZE USED= 16384
       66.125 MB WRITTEN ON ELEMENT SAVED DATA FILE: file0.esav
      102.125 MB WRITTEN ON ASSEMBLED MATRIX FILE: file0.full
       15.062 MB WRITTEN ON RESULTS FILE: file0.rst
 *************** Write FE CONNECTORS *********

 WRITE OUT CONSTRAINT EQUATIONS TO FILE= file.ce                                                                                                                                                                                                                                                             
 ****************************************************
 *************** FINISHED SOLVE FOR LS 1 *************

 *GET  _WALLASOL  FROM  ACTI  ITEM=TIME WALL  VALUE=  18.9463889    

 PRINTOUT RESUMED BY /GOP

 FINISH SOLUTION PROCESSING


 ***** ROUTINE COMPLETED *****  CP =        15.344



 *** ANSYS - ENGINEERING ANALYSIS SYSTEM  RELEASE Release 18.1     18.1     ***
 DISTRIBUTED ANSYS Multiphysics                                

 00000000  VERSION=WINDOWS x64   18:56:47  SEP 12, 2017 CP=     15.344

 unsaved_project--Static Structural (C5)                                       



          ***** ANSYS RESULTS INTERPRETATION (POST1) *****

 *** NOTE ***                            CP =      15.344   TIME= 18:56:47
 Reading results into the database (SET command) will update the current 
 displacement and force boundary conditions in the database with the     
 values from the results file for that load set.  Note that any          
 subsequent solutions will use these values unless action is taken to    
 either SAVE the current values or not overwrite them (/EXIT,NOSAVE).    

 Set Encoding of XML File to:ISO-8859-1

 Set Output of XML File to:
     PARM,     ,     ,     ,     ,     ,     ,     ,     ,     ,     ,     ,
         ,     ,     ,     ,     ,     ,     ,

 DATABASE WRITTEN ON FILE  parm.xml                                                                                                                                                                                                                                                            

 EXIT THE ANSYS POST1 DATABASE PROCESSOR


 ***** ROUTINE COMPLETED *****  CP =        15.344



 PRINTOUT RESUMED BY /GOP

 *GET  _WALLDONE  FROM  ACTI  ITEM=TIME WALL  VALUE=  18.9463889    

 PARAMETER _PREPTIME =     0.000000000    

 PARAMETER _SOLVTIME =     14.00000000    

 PARAMETER _POSTTIME =     0.000000000    

 PARAMETER _TOTALTIM =     14.00000000    

 EXIT ANSYS WITHOUT SAVING DATABASE


 NUMBER OF WARNING MESSAGES ENCOUNTERED=          3
 NUMBER OF ERROR   MESSAGES ENCOUNTERED=          0

+--------- D I S T R I B U T E D   A N S Y S   S T A T I S T I C S ------------+

Release: Release 18.1       Build: 18.1       Update: UP20170403   Platform: WINDOWS x64 
Date Run: 09/12/2017   Time: 18:56     Process ID: 4960
Operating System: Windows 8.1  (Build: 9600)

Processor Model: Intel(R) Xeon(R) CPU E3-1240 v3 @ 3.40GHz

Compiler: Intel(R) FORTRAN Compiler Version 15.0.7  (Build: 20160518)
          Intel(R) C/C++ Compiler Version 15.0.7  (Build: 20160518)
          Intel(R) Math Kernel Library Version 11.3.3 Product Build 20160413

Number of machines requested            :    1
Total number of cores available         :    8
Number of physical cores available      :    4
Number of processes requested           :    2
Number of threads per process requested :    1
Total number of cores requested         :    2 (Distributed Memory Parallel)               
MPI Type: INTELMPI
MPI Version: Intel(R) MPI Library 5.1.3 for Windows* OS


GPU Acceleration: Not Requested

Job Name: file0
Input File: dummy.dat

  Core                Machine Name   Working Directory
  ----------------------------------------------------
     0   Oleg-WS.TRANSMARINE.LOCAL   C:\Users\azer.b\AppData\Local\Temp\WB_OLEG-WS_Oleg.g_5632_2\_ProjectScratch\ScrC268
     1   Oleg-WS.TRANSMARINE.LOCAL   C:\Users\azer.b\AppData\Local\Temp\WB_OLEG-WS_Oleg.g_5632_2\_ProjectScratch\ScrC268
 
Latency time from master to core    1 =    0.700 microseconds
 
Communication speed from master to core    1 =  4239.55 MB/sec

Total CPU time for main thread                    :       14.0 seconds
Total CPU time summed for all threads             :       15.6 seconds

Elapsed time spent pre-processing model (/PREP7)  :        0.3 seconds
Elapsed time spent solution - preprocessing       :        0.9 seconds
Elapsed time spent computing solution             :       12.3 seconds
Elapsed time spent solution - postprocessing      :        0.1 seconds
Elapsed time spent post-processing model (/POST1) :        0.0 seconds
 
Equation solver used                              :            Sparse (symmetric)
Equation solver computational rate                :    33975.3 Mflops
Equation solver effective I/O rate                :    14159.8 MB/sec

Maximum total memory used                         :     2230.0 MB
Maximum total memory allocated                    :     4954.0 MB
Total physical memory available                   :         32 GB

+------ E N D   D I S T R I B U T E D   A N S Y S   S T A T I S T I C S -------+


 *---------------------------------------------------------------------------*
 |                                                                           |
 |                       DISTRIBUTED ANSYS RUN COMPLETED                     |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 | Ansys Release 18.1          Build 18.1         UP20170403     WINDOWS x64 |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 | Database Requested(-db)  1024 MB    Scratch Memory Requested      1024 MB |
 | Maximum Database Used      49 MB    Maximum Scratch Memory Used   1151 MB |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 |        CP Time      (sec) =         15.609       Time  =  18:56:48        |
 |        Elapsed Time (sec) =         17.000       Date  =  09/12/2017      |
 |                                                                           |
 *---------------------------------------------------------------------------*
