/COM,ANSYS RELEASE Release 18.1      BUILD 18.1      UP20170403       18:56:32

 *** WARNING ***                         CP =       0.781   TIME= 18:56:33
 Using 1 iteration per substep may result in unconverged solutions for   
 nonlinear analysis and the program may not indicate divergence in this  
 case.  Check your results.                                              

 *** WARNING ***                         CP =       0.844   TIME= 18:56:33
 Element shape checking is currently inactive.  Issue SHPP,ON or         
 SHPP,WARN to reactivate, if desired.                                    

 *** WARNING ***                         CP =       1.031   TIME= 18:56:33
 Material number 45 (used by element 28482 ) should normally have at     
 least one MP or one TB type command associated with it.  Output of      
 energy by material may not be available.                                
