/COM,ANSYS RELEASE Release 18.0      BUILD 18.0      UP20161219       21:15:57

 *** WARNING ***                         CP =       0.359   TIME= 21:15:58
 The program chosen initial timestep/load-factor is arbitrary.  It is    
 necessary for the user to supply a suitable initial                     
 timestep/load-factor through the NSUB or DELTIM command for             
 convergence and overall efficiency.                                     
